// SPDX-License-Identifier: GPL-2.0-or-later
/*
 * Copyright (c) 2019 Protonic Holland
 * Copyright (c) 2020 Oleksij Rempel <kernel@pengutronix.de>, Pengutronix
 */

/dts-v1/;
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/leds/common.h>
#include "imx6dl.dtsi"

/ {
	model = "Van der Laan LANMCU";
	compatible = "vdl,lanmcu", "fsl,imx6dl";

	chosen {
		stdout-path = &uart4;
	};

	clock_ksz8081: clock-ksz8081 {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <50000000>;
		clock-output-names = "enet_ref_pad";
	};

	backlight: backlight {
		compatible = "pwm-backlight";
		pwms = <&pwm1 0 5000000 0>;
		brightness-levels = <0 1000>;
		num-interpolated-steps = <20>;
		default-brightness-level = <19>;
	};

	display {
		compatible = "fsl,imx-parallel-display";
		pinctrl-0 = <&pinctrl_ipu1_disp>;
		pinctrl-names = "default";
		#address-cells = <1>;
		#size-cells = <0>;

		port@0 {
			reg = <0>;

			display_in: endpoint {
				remote-endpoint = <&ipu1_di0_disp0>;
			};
		};

		port@1 {
			reg = <1>;

			display_out: endpoint {
				remote-endpoint = <&panel_in>;
			};
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_leds>;

		led-0 {
			label = "debug0";
			function = LED_FUNCTION_STATUS;
			gpios = <&gpio1 8 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "heartbeat";
		};
	};

	panel {
		compatible = "edt,etm0700g0bdh6";
		backlight = <&backlight>;

		port {
			panel_in: endpoint {
				remote-endpoint = <&display_out>;
			};
		};
	};

	reg_otg_vbus: regulator-otg-vbus {
		compatible = "regulator-fixed";
		regulator-name = "otg-vbus";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gpio3 22 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};

	usdhc2_wifi_pwrseq: usdhc2-wifi-pwrseq {
		compatible = "mmc-pwrseq-simple";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_wifi_npd>;
		reset-gpios = <&gpio6 10 GPIO_ACTIVE_LOW>;
	};

};

&can1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_can1>;
	status = "okay";
};

&can2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_can2>;
	status = "okay";
};

&clks {
	clocks = <&clock_ksz8081>;
	clock-names = "enet_ref_pad";
	assigned-clocks = <&clks IMX6QDL_CLK_ENET_REF_SEL>;
	assigned-clock-parents = <&clock_ksz8081>;
};

&fec {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_enet>;
	phy-mode = "rmii";
	phy-handle = <&rgmii_phy>;
	status = "okay";

	mdio {
		#address-cells = <1>;
		#size-cells = <0>;

		/* Microchip KSZ8081RNA PHY */
		rgmii_phy: ethernet-phy@0 {
			reg = <0>;
			interrupts-extended = <&gpio5 23 IRQ_TYPE_LEVEL_LOW>;
			reset-gpios = <&gpio5 22 GPIO_ACTIVE_LOW>;
			reset-assert-us = <10000>;
			reset-deassert-us = <300>;
		};
	};
};

&gpio1 {
	gpio-line-names =
		"", "SD1_CD", "", "", "", "", "", "",
		"DEBUG_0", "BL_PWM", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "ENET_LED_GREEN",
		"", "", "", "", "", "", "", "";
};

&gpio3 {
	gpio-line-names =
		"", "", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "",
		"", "", "", "", "TS_INT", "USB_OTG1_OC", "USB_OTG1_PWR", "",
		"", "", "", "", "UART2_CTS", "", "UART3_CTS", "";
};

&gpio5 {
	gpio-line-names =
		"", "", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "",
		"", "", "", "", "", "", "ENET_RST", "ENET_INT",
		"", "", "I2C1_SDA", "I2C1_SCL", "", "", "", "";
};

&gpio6 {
	gpio-line-names =
		"", "", "", "", "", "", "", "",
		"", "", "WLAN_REG_ON", "", "", "", "", "",
		"", "", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "";
};

&gpio7 {
	gpio-line-names =
		"", "", "", "", "", "", "", "",
		"EMMC_RST", "", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "";
};

&i2c1 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c1>;
	status = "okay";

	/* additional i2c devices are added automatically by the boot loader */
};

&i2c3 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c3>;
	status = "okay";

	touchscreen@38 {
		compatible = "edt,edt-ft5406";
		reg = <0x38>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_ts_edt>;
		interrupts-extended = <&gpio3 20 IRQ_TYPE_EDGE_FALLING>;

		touchscreen-size-x = <1792>;
		touchscreen-size-y = <1024>;

		touchscreen-fuzz-x = <0>;
		touchscreen-fuzz-y = <0>;

		/* Touch screen calibration */
		threshold = <50>;
		gain = <5>;
		offset = <10>;
	};

	rtc@51 {
		compatible = "nxp,pcf8563";
		reg = <0x51>;
	};
};

&ipu1_di0_disp0 {
	remote-endpoint = <&display_in>;
};

&pwm1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_pwm1>;
	status = "okay";
};

&uart2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart2>;
	linux,rs485-enabled-at-boot-time;
	uart-has-rtscts;
	status = "okay";
};

&uart3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart3>;
	linux,rs485-enabled-at-boot-time;
	uart-has-rtscts;
	status = "okay";
};

&uart4 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart4>;
	status = "okay";
};

&usbotg {
	vbus-supply = <&reg_otg_vbus>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usbotg>;
	phy_type = "utmi";
	dr_mode = "host";
	over-current-active-low;
	status = "okay";
};

&usbphynop1 {
	status = "disabled";
};

&usbphynop2 {
	status = "disabled";
};

&usdhc1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc1>;
	cd-gpios = <&gpio1 1 GPIO_ACTIVE_LOW>;
	no-1-8-v;
	disable-wp;
	cap-sd-highspeed;
	no-mmc;
	no-sdio;
	status = "okay";
};

&usdhc2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc2>;
	no-1-8-v;
	non-removable;
	mmc-pwrseq = <&usdhc2_wifi_pwrseq>;
	#address-cells = <1>;
	#size-cells = <0>;
	status = "okay";

	wifi@1 {
		reg = <1>;
		compatible = "brcm,bcm4329-fmac";
	};
};

&usdhc3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc3>;
	bus-width = <8>;
	no-1-8-v;
	non-removable;
	no-sd;
	no-sdio;
	status = "okay";
};

&iomuxc {
	pinctrl_can1: can1grp {
		fsl,pins = <
			MX6QDL_PAD_KEY_ROW2__FLEXCAN1_RX		0x1b000
			MX6QDL_PAD_KEY_COL2__FLEXCAN1_TX		0x3008
		>;
	};

	pinctrl_can2: can2grp {
		fsl,pins = <
			MX6QDL_PAD_KEY_ROW4__FLEXCAN2_RX		0x1b000
			MX6QDL_PAD_KEY_COL4__FLEXCAN2_TX		0x3008
		>;
	};

	pinctrl_enet: enetgrp {
		fsl,pins = <
			/* MX6QDL_ENET_PINGRP4 */
			MX6QDL_PAD_ENET_MDC__ENET_MDC			0x1b0b0
			MX6QDL_PAD_ENET_MDIO__ENET_MDIO			0x1b0b0
			MX6QDL_PAD_ENET_RXD0__ENET_RX_DATA0		0x1b0b0
			MX6QDL_PAD_ENET_RXD1__ENET_RX_DATA1		0x1b0b0
			MX6QDL_PAD_ENET_RX_ER__ENET_RX_ER		0x1b0b0
			MX6QDL_PAD_ENET_TX_EN__ENET_TX_EN		0x1b0b0
			MX6QDL_PAD_ENET_TXD0__ENET_TX_DATA0		0x1b0b0
			MX6QDL_PAD_ENET_TXD1__ENET_TX_DATA1		0x1b0b0
			MX6QDL_PAD_ENET_CRS_DV__ENET_RX_EN		0x1b0b0

			MX6QDL_PAD_GPIO_16__ENET_REF_CLK		0x1b0b0
			/* Phy reset */
			MX6QDL_PAD_CSI0_DAT4__GPIO5_IO22		0x1b0b0
			/* nINTRP */
			MX6QDL_PAD_CSI0_DAT5__GPIO5_IO23		0x1b0b0
		>;
	};

	pinctrl_i2c1: i2c1grp {
		fsl,pins = <
			MX6QDL_PAD_CSI0_DAT8__I2C1_SDA			0x4001f8b1
			MX6QDL_PAD_CSI0_DAT9__I2C1_SCL			0x4001f8b1
		>;
	};

	pinctrl_i2c3: i2c3grp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_5__I2C3_SCL			0x4001b8b1
			MX6QDL_PAD_GPIO_6__I2C3_SDA			0x4001b8b1
		>;
	};

	pinctrl_ipu1_disp: ipudisp1grp {
		fsl,pins = <
			/* DSE 0x30 => 25 Ohm, 0x20 => 37 Ohm, 0x10 => 75 Ohm */
			MX6QDL_PAD_DI0_DISP_CLK__IPU1_DI0_DISP_CLK	0x30
			MX6QDL_PAD_DI0_PIN2__IPU1_DI0_PIN02		0x30
			MX6QDL_PAD_DI0_PIN3__IPU1_DI0_PIN03		0x30
			MX6QDL_PAD_DI0_PIN15__IPU1_DI0_PIN15		0x30
			MX6QDL_PAD_DISP0_DAT0__IPU1_DISP0_DATA00	0x30
			MX6QDL_PAD_DISP0_DAT1__IPU1_DISP0_DATA01	0x30
			MX6QDL_PAD_DISP0_DAT2__IPU1_DISP0_DATA02	0x30
			MX6QDL_PAD_DISP0_DAT3__IPU1_DISP0_DATA03	0x30
			MX6QDL_PAD_DISP0_DAT4__IPU1_DISP0_DATA04	0x30
			MX6QDL_PAD_DISP0_DAT5__IPU1_DISP0_DATA05	0x30
			MX6QDL_PAD_DISP0_DAT6__IPU1_DISP0_DATA06	0x30
			MX6QDL_PAD_DISP0_DAT7__IPU1_DISP0_DATA07	0x30
			MX6QDL_PAD_DISP0_DAT8__IPU1_DISP0_DATA08	0x30
			MX6QDL_PAD_DISP0_DAT9__IPU1_DISP0_DATA09	0x30
			MX6QDL_PAD_DISP0_DAT10__IPU1_DISP0_DATA10	0x30
			MX6QDL_PAD_DISP0_DAT11__IPU1_DISP0_DATA11	0x30
			MX6QDL_PAD_DISP0_DAT12__IPU1_DISP0_DATA12	0x30
			MX6QDL_PAD_DISP0_DAT13__IPU1_DISP0_DATA13	0x30
			MX6QDL_PAD_DISP0_DAT14__IPU1_DISP0_DATA14	0x30
			MX6QDL_PAD_DISP0_DAT15__IPU1_DISP0_DATA15	0x30
			MX6QDL_PAD_DISP0_DAT16__IPU1_DISP0_DATA16	0x30
			MX6QDL_PAD_DISP0_DAT17__IPU1_DISP0_DATA17	0x30
		>;
	};

	pinctrl_leds: ledsgrp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_8__GPIO1_IO08			0x1b0b0
		>;
	};

	pinctrl_pwm1: pwm1grp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_9__PWM1_OUT			0x8
		>;
	};

	pinctrl_ts_edt: ts1grp {
		fsl,pins = <
			MX6QDL_PAD_EIM_D20__GPIO3_IO20			0x1b0b0
		>;
	};

	pinctrl_uart2: uart2grp {
		fsl,pins = <
			MX6QDL_PAD_EIM_D26__UART2_RX_DATA		0x1b0b1
			MX6QDL_PAD_EIM_D27__UART2_TX_DATA		0x1b0b1
			MX6QDL_PAD_EIM_D28__UART2_CTS_B			0x130b1
		>;
	};

	pinctrl_uart3: uart3grp {
		fsl,pins = <
			MX6QDL_PAD_EIM_D24__UART3_TX_DATA		0x1b0b1
			MX6QDL_PAD_EIM_D25__UART3_RX_DATA		0x1b0b1
			MX6QDL_PAD_EIM_D30__UART3_CTS_B			0x130b1
		>;
	};

	pinctrl_uart4: uart4grp {
		fsl,pins = <
			MX6QDL_PAD_KEY_COL0__UART4_TX_DATA		0x1b0b1
			MX6QDL_PAD_KEY_ROW0__UART4_RX_DATA		0x1b0b1
		>;
	};

	pinctrl_usbotg: usbotggrp {
		fsl,pins = <
			MX6QDL_PAD_EIM_D21__USB_OTG_OC			0x1b0b0
			/* power enable, high active */
			MX6QDL_PAD_EIM_D22__GPIO3_IO22			0x1b0b0
		>;
	};

	pinctrl_usdhc1: usdhc1grp {
		fsl,pins = <
			MX6QDL_PAD_SD1_CMD__SD1_CMD			0x170f9
			MX6QDL_PAD_SD1_CLK__SD1_CLK			0x100f9
			MX6QDL_PAD_SD1_DAT0__SD1_DATA0			0x170f9
			MX6QDL_PAD_SD1_DAT1__SD1_DATA1			0x170f9
			MX6QDL_PAD_SD1_DAT2__SD1_DATA2			0x170f9
			MX6QDL_PAD_SD1_DAT3__SD1_DATA3			0x170f9
			MX6QDL_PAD_GPIO_1__SD1_CD_B			0x1b0b0
		>;
	};

	pinctrl_usdhc2: usdhc2grp {
		fsl,pins = <
			MX6QDL_PAD_SD2_CMD__SD2_CMD			0x170b9
			MX6QDL_PAD_SD2_CLK__SD2_CLK			0x100b9
			MX6QDL_PAD_SD2_DAT0__SD2_DATA0			0x170b9
			MX6QDL_PAD_SD2_DAT1__SD2_DATA1			0x170b9
			MX6QDL_PAD_SD2_DAT2__SD2_DATA2			0x170b9
			MX6QDL_PAD_SD2_DAT3__SD2_DATA3			0x170b9
		>;
	};

	pinctrl_usdhc3: usdhc3grp {
		fsl,pins = <
			MX6QDL_PAD_SD3_CMD__SD3_CMD			0x17099
			MX6QDL_PAD_SD3_CLK__SD3_CLK			0x10099
			MX6QDL_PAD_SD3_DAT0__SD3_DATA0			0x17099
			MX6QDL_PAD_SD3_DAT1__SD3_DATA1			0x17099
			MX6QDL_PAD_SD3_DAT2__SD3_DATA2			0x17099
			MX6QDL_PAD_SD3_DAT3__SD3_DATA3			0x17099
			MX6QDL_PAD_SD3_DAT4__SD3_DATA4			0x17099
			MX6QDL_PAD_SD3_DAT5__SD3_DATA5			0x17099
			MX6QDL_PAD_SD3_DAT6__SD3_DATA6			0x17099
			MX6QDL_PAD_SD3_DAT7__SD3_DATA7			0x17099
			MX6QDL_PAD_SD3_RST__SD3_RESET			0x1b0b1
		>;
	};

	pinctrl_wifi_npd: wifigrp {
		fsl,pins = <
			/* WL_REG_ON */
			MX6QDL_PAD_NANDF_RB0__GPIO6_IO10		0x13069
		>;
	};
};
