/*
 * support for the imx6 based aristainetos2 board
 *
 * Copyright (C) 2015 Heiko Schocher <hs@denx.de>
 *
 * This file is dual-licensed: you can use it either under the terms
 * of the GPL or the X11 license, at your option. Note that this dual
 * licensing only applies to this file, and not this project as a
 * whole.
 *
 *  a) This file is free software; you can redistribute it and/or
 *     modify it under the terms of the GNU General Public License
 *     version 2 as published by the Free Software Foundation.
 *
 *     This file is distributed in the hope that it will be useful,
 *     but WITHOUT ANY WARRANTY; without even the implied warranty of
 *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 *     GNU General Public License for more details.
 *
 * Or, alternatively,
 *
 *  b) Permission is hereby granted, free of charge, to any person
 *     obtaining a copy of this software and associated documentation
 *     files (the "Software"), to deal in the Software without
 *     restriction, including without limitation the rights to use,
 *     copy, modify, merge, publish, distribute, sublicense, and/or
 *     sell copies of the Software, and to permit persons to whom the
 *     Software is furnished to do so, subject to the following
 *     conditions:
 *
 *     The above copyright notice and this permission notice shall be
 *     included in all copies or substantial portions of the Software.
 *
 *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
 *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
 *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
 *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
 *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
 *     OTHER DEALINGS IN THE SOFTWARE.
 */
/dts-v1/;
#include "imx6dl.dtsi"
#include "imx6qdl-aristainetos2.dtsi"

/ {
	model = "aristainetos2 i.MX6 Dual Lite Board 7";
	compatible = "abb,aristainetos2-imx6dl-7", "fsl,imx6dl";

	memory@10000000 {
		device_type = "memory";
		reg = <0x10000000 0x40000000>;
	};

	panel: panel {
		compatible = "lg,lb070wv8";
		backlight = <&backlight>;
		enable-gpios = <&gpio6 15 GPIO_ACTIVE_HIGH>;

		port {
			panel_in: endpoint {
				remote-endpoint = <&lvds0_out>;
			};
		};
	};
};

&i2c3 {
	touch: touch@4d {
		compatible = "atmel,maxtouch";
		reg = <0x4d>;
		interrupt-parent = <&gpio2>;
		interrupts = <9 8>;
	};
};

&ldb {
	status = "okay";

	lvds-channel@0 {
		status = "okay";

		port@0 {
			reg = <0>;
			lvds0_in: endpoint {
				remote-endpoint = <&ipu1_di0_lvds0>;
			};
		};

		port@4 {
			reg = <4>;
			lvds0_out: endpoint {
				remote-endpoint = <&panel_in>;
			};
		};
	};
};
