/*
 * Copyright 2015 Timesys Corporation.
 * Copyright 2015 General Electric Company
 *
 * This file is dual-licensed: you can use it either under the terms
 * of the GPL or the X11 license, at your option. Note that this dual
 * licensing only applies to this file, and not this project as a
 * whole.
 *
 *  a) This file is free software; you can redistribute it and/or
 *     modify it under the terms of the GNU General Public License
 *     version 2 as published by the Free Software Foundation.
 *
 *     This file is distributed in the hope that it will be useful,
 *     but WITHOUT ANY WARRANTY; without even the implied warranty of
 *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 *     GNU General Public License for more details.
 *
 * Or, alternatively,
 *
 *  b) Permission is hereby granted, free of charge, to any person
 *     obtaining a copy of this software and associated documentation
 *     files (the "Software"), to deal in the Software without
 *     restriction, including without limitation the rights to use,
 *     copy, modify, merge, publish, distribute, sublicense, and/or
 *     sell copies of the Software, and to permit persons to whom the
 *     Software is furnished to do so, subject to the following
 *     conditions:
 *
 *     The above copyright notice and this permission notice shall be
 *     included in all copies or substantial portions of the Software.
 *
 *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
 *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
 *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
 *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
 *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
 *     OTHER DEALINGS IN THE SOFTWARE.
 */

#include "imx6q-ba16.dtsi"

/ {
	mclk: clock-mclk {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <22000000>;
	};

	gpio-poweroff {
		compatible = "gpio-poweroff";
		gpios = <&gpio4 11 GPIO_ACTIVE_LOW>;
		status = "okay";
	};

	reg_wl18xx_vmmc: regulator-wl18xx {
		compatible = "regulator-fixed";
		regulator-name = "vwl1807";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		gpio = <&pca9539 3 GPIO_ACTIVE_HIGH>;
		startup-delay-us = <70000>;
		enable-active-high;
	};

	reg_wlan: regulator-wlan {
		compatible = "regulator-fixed";
		regulator-name = "3P3V_wlan";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
		regulator-boot-on;
		gpio = <&gpio6 14 GPIO_ACTIVE_HIGH>;
	};

	sound {
		compatible = "fsl,imx6q-ba16-sgtl5000",
			     "fsl,imx-audio-sgtl5000";
		model = "imx6q-ba16-sgtl5000";
		ssi-controller = <&ssi1>;
		audio-codec = <&sgtl5000>;
		audio-routing =
			"MIC_IN", "Mic Jack",
			"Mic Jack", "Mic Bias",
			"LINE_IN", "Line In Jack",
			"Headphone Jack", "HP_OUT";
		mux-int-port = <1>;
		mux-ext-port = <4>;
	};

	aliases {
		mdio-gpio0 = &mdio0;
	};

	mdio0: mdio-gpio {
		compatible = "virtual,mdio-gpio";
		gpios = <&gpio2 5 GPIO_ACTIVE_HIGH>, /* mdc */
			<&gpio2 7 GPIO_ACTIVE_HIGH>; /* mdio */

		#address-cells = <1>;
		#size-cells = <0>;

		switch: switch@0 {
			compatible = "marvell,mv88e6085"; /* 88e6240*/
			reg = <0>;

			interrupt-parent = <&gpio2>;
			interrupts = <2 IRQ_TYPE_LEVEL_LOW>;
			interrupt-controller;
			#interrupt-cells = <2>;

			switch_ports: ports {
				#address-cells = <1>;
				#size-cells = <0>;
			};

			mdio {
				#address-cells = <1>;
				#size-cells = <0>;

				switchphy0: switchphy@0 {
					reg = <0>;
					interrupt-parent = <&switch>;
					interrupts = <0 IRQ_TYPE_LEVEL_HIGH>;
				};

				switchphy1: switchphy@1 {
					reg = <1>;
					interrupt-parent = <&switch>;
					interrupts = <1 IRQ_TYPE_LEVEL_HIGH>;
				};

				switchphy2: switchphy@2 {
					reg = <2>;
					interrupt-parent = <&switch>;
					interrupts = <2 IRQ_TYPE_LEVEL_HIGH>;
				};

				switchphy3: switchphy@3 {
					reg = <3>;
					interrupt-parent = <&switch>;
					interrupts = <3 IRQ_TYPE_LEVEL_HIGH>;
				};

				switchphy4: switchphy@4 {
					reg = <4>;
					interrupt-parent = <&switch>;
					interrupts = <4 IRQ_TYPE_LEVEL_HIGH>;
				};
			};
		};
	};
};

&ecspi5 {
	cs-gpios = <&gpio1 17 GPIO_ACTIVE_LOW>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_ecspi5>;
	status = "okay";

	m25_eeprom: flash@0 {
		compatible = "atmel,at25";
		spi-max-frequency = <10000000>;
		size = <0x8000>;
		pagesize = <64>;
		reg = <0>;
		address-width = <16>;
	};
};

&i2c1 {
	pinctrl-names = "default", "gpio";
	pinctrl-1 = <&pinctrl_i2c1_gpio>;
	sda-gpios = <&gpio5 26 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
	scl-gpios = <&gpio5 27 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;

	pca9547: mux@70 {
		compatible = "nxp,pca9547";
		reg = <0x70>;
		#address-cells = <1>;
		#size-cells = <0>;

		mux1_i2c1: i2c@0 {
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0>;

			ads7830: ads7830@48 {
				compatible = "ti,ads7830";
				reg = <0x48>;
			};

			mma8453: mma8453@1c {
				compatible = "fsl,mma8453";
				reg = <0x1c>;
			};
		};

		mux1_i2c2: i2c@1 {
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x1>;

			eeprom: eeprom@50 {
				compatible = "atmel,24c08";
				reg = <0x50>;
			};

			mpl3115: mpl3115@60 {
				compatible = "fsl,mpl3115";
				reg = <0x60>;
			};
		};

		mux1_i2c3: i2c@2 {
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x2>;
		};

		mux1_i2c4: i2c@3 {
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x3>;

			sgtl5000: codec@a {
				compatible = "fsl,sgtl5000";
				reg = <0x0a>;
				#sound-dai-cells = <0>;
				clocks = <&mclk>;
				VDDA-supply = <&reg_1p8v>;
				VDDIO-supply = <&reg_3p3v>;
			};
		};

		mux1_i2c5: i2c@4 {
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x4>;

			pca9539: pca9539@74 {
				compatible = "nxp,pca9539";
				reg = <0x74>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				interrupt-parent = <&gpio2>;
				interrupts = <3 IRQ_TYPE_LEVEL_LOW>;

				P12-hog {
					gpio-hog;
					gpios = <10 0>;
					output-low;
					line-name = "PCA9539-P12";
				};

				P13-hog {
					gpio-hog;
					gpios = <11 0>;
					output-low;
					line-name = "PCA9539-P13";
				};

				P14-hog {
					gpio-hog;
					gpios = <12 0>;
					output-low;
					line-name = "PCA9539-P14";
				};

				P15-hog {
					gpio-hog;
					gpios = <13 0>;
					output-low;
					line-name = "PCA9539-P15";
				};

				P16-hog {
					gpio-hog;
					gpios = <14 0>;
					output-low;
					line-name = "PCA9539-P16";
				};

				P17-hog {
					gpio-hog;
					gpios = <15 0>;
					output-low;
					line-name = "PCA9539-P17";
				};
			};
		};

		mux1_i2c6: i2c@5 {
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x5>;
		};

		mux1_i2c7: i2c@6 {
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x6>;
		};

		mux1_i2c8: i2c@7 {
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x7>;
		};
	};
};

&i2c2 {
	pinctrl-names = "default", "gpio";
	pinctrl-1 = <&pinctrl_i2c2_gpio>;
	sda-gpios = <&gpio4 13 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
	scl-gpios = <&gpio4 12 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
};

&i2c3 {
	pinctrl-names = "default", "gpio";
	pinctrl-1 = <&pinctrl_i2c3_gpio>;
	sda-gpios = <&gpio1 6 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
	scl-gpios = <&gpio1 3 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
};

&iomuxc {
	pinctrl_i2c1_gpio: i2c1gpiogrp {
		fsl,pins = <
			MX6QDL_PAD_CSI0_DAT8__GPIO5_IO26	0x1b0b0
			MX6QDL_PAD_CSI0_DAT9__GPIO5_IO27	0x1b0b0
		>;
	};

	pinctrl_i2c2_gpio: i2c2gpiogrp {
		fsl,pins = <
			MX6QDL_PAD_KEY_COL3__GPIO4_IO12	0x1b0b0
			MX6QDL_PAD_KEY_ROW3__GPIO4_IO13	0x1b0b0
		>;
	};

	pinctrl_i2c3_gpio: i2c3gpiogrp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_3__GPIO1_IO03	0x1b0b0
			MX6QDL_PAD_GPIO_6__GPIO1_IO06	0x1b0b0
		>;
	};
};

&pmu {
	secure-reg-access;
};

&usdhc2 {
	status = "disabled";
};

&usdhc4 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc4>;
	bus-width = <4>;
	vmmc-supply = <&reg_wl18xx_vmmc>;
	no-1-8-v;
	non-removable;
	wakeup-source;
	keep-power-in-suspend;
	cap-power-off-card;
	max-frequency = <25000000>;
	#address-cells = <1>;
	#size-cells = <0>;
	status = "okay";

	wlcore: wlcore@2 {
		compatible = "ti,wl1837";
		reg = <2>;
		interrupt-parent = <&gpio2>;
		interrupts = <6 IRQ_TYPE_LEVEL_HIGH>;
		tcxo-clock-frequency = <26000000>;
	};
};

&pcie {
	/* Synopsys, Inc. Device */
	pci_root: root@0,0 {
		compatible = "pci16c3,abcd";
		reg = <0x00000000 0 0 0 0>;

		#address-cells = <3>;
		#size-cells = <2>;
		#interrupt-cells = <1>;
	};
};

&clks {
	assigned-clocks = <&clks IMX6QDL_CLK_LDB_DI0_SEL>,
			  <&clks IMX6QDL_CLK_LDB_DI1_SEL>,
			  <&clks IMX6QDL_CLK_IPU1_DI0_PRE_SEL>,
			  <&clks IMX6QDL_CLK_IPU1_DI1_PRE_SEL>,
			  <&clks IMX6QDL_CLK_IPU2_DI0_PRE_SEL>,
			  <&clks IMX6QDL_CLK_IPU2_DI1_PRE_SEL>;
	assigned-clock-parents = <&clks IMX6QDL_CLK_PLL5_VIDEO_DIV>,
				 <&clks IMX6QDL_CLK_PLL5_VIDEO_DIV>,
				 <&clks IMX6QDL_CLK_PLL2_PFD0_352M>,
				 <&clks IMX6QDL_CLK_PLL2_PFD0_352M>,
				 <&clks IMX6QDL_CLK_PLL2_PFD0_352M>,
				 <&clks IMX6QDL_CLK_PLL2_PFD0_352M>;
};
