// SPDX-License-Identifier: (GPL-2.0)
/*
 * Device tree for the Kobo Clara HD ebook reader
 *
 * Name on mainboard is: 37NB-E60K00+4A4
 * Serials start with: E60K02 (a number also seen in
 * vendor kernel sources)
 *
 * This mainboard seems to be equipped with different SoCs.
 * In the Kobo Clara HD ebook reader it is an i.MX6SLL
 *
 * Copyright 2019 Andreas Kemnade
 * based on works
 * Copyright 2016 Freescale Semiconductor, Inc.
 */

/dts-v1/;

#include <dt-bindings/input/input.h>
#include <dt-bindings/gpio/gpio.h>
#include "imx6sll.dtsi"
#include "e60k02.dtsi"

/ {
	model = "Kobo Clara HD";
	compatible = "kobo,clarahd", "fsl,imx6sll";
};

&clks {
	assigned-clocks = <&clks IMX6SLL_CLK_PLL4_AUDIO_DIV>;
	assigned-clock-rates = <393216000>;
};

&cpu0 {
	arm-supply = <&dcdc3_reg>;
	soc-supply = <&dcdc1_reg>;
};

&gpio_keys {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_gpio_keys>;
};

&i2c1 {
	pinctrl-names = "default","sleep";
	pinctrl-0 = <&pinctrl_i2c1>;
	pinctrl-1 = <&pinctrl_i2c1_sleep>;
};

&i2c2 {
	pinctrl-names = "default","sleep";
	pinctrl-0 = <&pinctrl_i2c2>;
	pinctrl-1 = <&pinctrl_i2c2_sleep>;
};

&i2c3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c3>;
};

&iomuxc {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_hog>;

	pinctrl_cyttsp5_gpio: cyttsp5-gpiogrp {
		fsl,pins = <
			MX6SLL_PAD_SD1_DATA3__GPIO5_IO06                0x17059 /* TP_INT */
			MX6SLL_PAD_SD1_DATA2__GPIO5_IO13                0x10059 /* TP_RST */
		>;
	};

	pinctrl_gpio_keys: gpio-keysgrp {
		fsl,pins = <
			MX6SLL_PAD_SD1_DATA1__GPIO5_IO08	0x17059	/* PWR_SW */
			MX6SLL_PAD_SD1_DATA4__GPIO5_IO12	0x17059	/* HALL_EN */
		>;
	};

	pinctrl_hog: hoggrp {
		fsl,pins = <
			MX6SLL_PAD_LCD_DATA00__GPIO2_IO20	0x79
			MX6SLL_PAD_LCD_DATA01__GPIO2_IO21	0x79
			MX6SLL_PAD_LCD_DATA02__GPIO2_IO22	0x79
			MX6SLL_PAD_LCD_DATA03__GPIO2_IO23	0x79
			MX6SLL_PAD_LCD_DATA04__GPIO2_IO24	0x79
			MX6SLL_PAD_LCD_DATA05__GPIO2_IO25	0x79
			MX6SLL_PAD_LCD_DATA06__GPIO2_IO26	0x79
			MX6SLL_PAD_LCD_DATA07__GPIO2_IO27	0x79
			MX6SLL_PAD_LCD_DATA08__GPIO2_IO28	0x79
			MX6SLL_PAD_LCD_DATA09__GPIO2_IO29	0x79
			MX6SLL_PAD_LCD_DATA10__GPIO2_IO30	0x79
			MX6SLL_PAD_LCD_DATA11__GPIO2_IO31	0x79
			MX6SLL_PAD_LCD_DATA12__GPIO3_IO00	0x79
			MX6SLL_PAD_LCD_DATA13__GPIO3_IO01	0x79
			MX6SLL_PAD_LCD_DATA14__GPIO3_IO02	0x79
			MX6SLL_PAD_LCD_DATA15__GPIO3_IO03	0x79
			MX6SLL_PAD_LCD_DATA16__GPIO3_IO04	0x79
			MX6SLL_PAD_LCD_DATA17__GPIO3_IO05	0x79
			MX6SLL_PAD_LCD_DATA18__GPIO3_IO06	0x79
			MX6SLL_PAD_LCD_DATA19__GPIO3_IO07	0x79
			MX6SLL_PAD_LCD_DATA20__GPIO3_IO08	0x79
			MX6SLL_PAD_LCD_DATA21__GPIO3_IO09	0x79
			MX6SLL_PAD_LCD_DATA22__GPIO3_IO10	0x79
			MX6SLL_PAD_LCD_DATA23__GPIO3_IO11	0x79
			MX6SLL_PAD_LCD_CLK__GPIO2_IO15		0x79
			MX6SLL_PAD_LCD_ENABLE__GPIO2_IO16	0x79
			MX6SLL_PAD_LCD_HSYNC__GPIO2_IO17	0x79
			MX6SLL_PAD_LCD_VSYNC__GPIO2_IO18	0x79
			MX6SLL_PAD_LCD_RESET__GPIO2_IO19	0x79
			MX6SLL_PAD_KEY_COL3__GPIO3_IO30		0x79
			MX6SLL_PAD_KEY_ROW7__GPIO4_IO07		0x79
			MX6SLL_PAD_ECSPI2_MOSI__GPIO4_IO13	0x79
			MX6SLL_PAD_KEY_COL5__GPIO4_IO02		0x79
		>;
	};

	pinctrl_i2c1: i2c1grp {
		fsl,pins = <
			MX6SLL_PAD_I2C1_SCL__I2C1_SCL	0x4001f8b1
			MX6SLL_PAD_I2C1_SDA__I2C1_SDA	0x4001f8b1
		>;
	};

	pinctrl_i2c1_sleep: i2c1grp-sleep {
		fsl,pins = <
			MX6SLL_PAD_I2C1_SCL__I2C1_SCL	0x400108b1
			MX6SLL_PAD_I2C1_SDA__I2C1_SDA	0x400108b1
		>;
	};

	pinctrl_i2c2: i2c2grp {
		fsl,pins = <
			MX6SLL_PAD_I2C2_SCL__I2C2_SCL	0x4001f8b1
			MX6SLL_PAD_I2C2_SDA__I2C2_SDA	0x4001f8b1
		>;
	};

	pinctrl_i2c2_sleep: i2c2grp-sleep {
		fsl,pins = <
			MX6SLL_PAD_I2C2_SCL__I2C2_SCL	0x400108b1
			MX6SLL_PAD_I2C2_SDA__I2C2_SDA	0x400108b1
		>;
	};

	pinctrl_i2c3: i2c3grp {
		fsl,pins = <
			MX6SLL_PAD_REF_CLK_24M__I2C3_SCL 0x4001f8b1
			MX6SLL_PAD_REF_CLK_32K__I2C3_SDA 0x4001f8b1
		>;
	};

	pinctrl_led: ledgrp {
		fsl,pins = <
			MX6SLL_PAD_SD1_DATA6__GPIO5_IO07 0x17059
		>;
	};

	pinctrl_lm3630a_bl_gpio: lm3630a-bl-gpiogrp {
		fsl,pins = <
			MX6SLL_PAD_EPDC_PWR_CTRL3__GPIO2_IO10	0x10059 /* HWEN */
		>;
	};

	pinctrl_ricoh_gpio: ricoh-gpiogrp {
		fsl,pins = <
			MX6SLL_PAD_SD1_CLK__GPIO5_IO15	0x1b8b1 /* ricoh619 chg */
			MX6SLL_PAD_SD1_DATA0__GPIO5_IO11 0x1b8b1 /* ricoh619 irq */
			MX6SLL_PAD_KEY_COL2__GPIO3_IO28	0x1b8b1 /* ricoh619 bat_low_int */
		>;
	};

	pinctrl_uart1: uart1grp {
		fsl,pins = <
			MX6SLL_PAD_UART1_TXD__UART1_DCE_TX 0x1b0b1
			MX6SLL_PAD_UART1_RXD__UART1_DCE_RX 0x1b0b1
		>;
	};

	pinctrl_uart4: uart4grp {
		fsl,pins = <
			MX6SLL_PAD_KEY_ROW6__UART4_DCE_TX 0x1b0b1
			MX6SLL_PAD_KEY_COL6__UART4_DCE_RX 0x1b0b1
		>;
	};

	pinctrl_usbotg1: usbotg1grp {
		fsl,pins = <
			MX6SLL_PAD_EPDC_PWR_COM__USB_OTG1_ID 0x17059
		>;
	};

	pinctrl_usdhc2: usdhc2grp {
		fsl,pins = <
			MX6SLL_PAD_SD2_CMD__SD2_CMD		0x17059
			MX6SLL_PAD_SD2_CLK__SD2_CLK		0x13059
			MX6SLL_PAD_SD2_DATA0__SD2_DATA0		0x17059
			MX6SLL_PAD_SD2_DATA1__SD2_DATA1		0x17059
			MX6SLL_PAD_SD2_DATA2__SD2_DATA2		0x17059
			MX6SLL_PAD_SD2_DATA3__SD2_DATA3		0x17059
		>;
	};

	pinctrl_usdhc2_100mhz: usdhc2grp-100mhz {
		fsl,pins = <
			MX6SLL_PAD_SD2_CMD__SD2_CMD		0x170b9
			MX6SLL_PAD_SD2_CLK__SD2_CLK		0x130b9
			MX6SLL_PAD_SD2_DATA0__SD2_DATA0		0x170b9
			MX6SLL_PAD_SD2_DATA1__SD2_DATA1		0x170b9
			MX6SLL_PAD_SD2_DATA2__SD2_DATA2		0x170b9
			MX6SLL_PAD_SD2_DATA3__SD2_DATA3		0x170b9
		>;
	};

	pinctrl_usdhc2_200mhz: usdhc2grp-200mhz {
		fsl,pins = <
			MX6SLL_PAD_SD2_CMD__SD2_CMD		0x170f9
			MX6SLL_PAD_SD2_CLK__SD2_CLK		0x130f9
			MX6SLL_PAD_SD2_DATA0__SD2_DATA0		0x170f9
			MX6SLL_PAD_SD2_DATA1__SD2_DATA1		0x170f9
			MX6SLL_PAD_SD2_DATA2__SD2_DATA2		0x170f9
			MX6SLL_PAD_SD2_DATA3__SD2_DATA3		0x170f9
		>;
	};

	pinctrl_usdhc2_sleep: usdhc2grp-sleep {
		fsl,pins = <
			MX6SLL_PAD_SD2_CMD__GPIO5_IO04		0x100f9
			MX6SLL_PAD_SD2_CLK__GPIO5_IO05		0x100f9
			MX6SLL_PAD_SD2_DATA0__GPIO5_IO01	0x100f9
			MX6SLL_PAD_SD2_DATA1__GPIO4_IO30	0x100f9
			MX6SLL_PAD_SD2_DATA2__GPIO5_IO03	0x100f9
			MX6SLL_PAD_SD2_DATA3__GPIO4_IO28	0x100f9
		>;
	};

	pinctrl_usdhc3: usdhc3grp {
		fsl,pins = <
			MX6SLL_PAD_SD3_CMD__SD3_CMD	0x11059
			MX6SLL_PAD_SD3_CLK__SD3_CLK	0x11059
			MX6SLL_PAD_SD3_DATA0__SD3_DATA0	0x11059
			MX6SLL_PAD_SD3_DATA1__SD3_DATA1	0x11059
			MX6SLL_PAD_SD3_DATA2__SD3_DATA2	0x11059
			MX6SLL_PAD_SD3_DATA3__SD3_DATA3	0x11059
		>;
	};

	pinctrl_usdhc3_100mhz: usdhc3grp-100mhz {
		fsl,pins = <
			MX6SLL_PAD_SD3_CMD__SD3_CMD	0x170b9
			MX6SLL_PAD_SD3_CLK__SD3_CLK	0x170b9
			MX6SLL_PAD_SD3_DATA0__SD3_DATA0	0x170b9
			MX6SLL_PAD_SD3_DATA1__SD3_DATA1	0x170b9
			MX6SLL_PAD_SD3_DATA2__SD3_DATA2	0x170b9
			MX6SLL_PAD_SD3_DATA3__SD3_DATA3	0x170b9
		>;
	};

	pinctrl_usdhc3_200mhz: usdhc3grp-200mhz {
		fsl,pins = <
			MX6SLL_PAD_SD3_CMD__SD3_CMD	0x170f9
			MX6SLL_PAD_SD3_CLK__SD3_CLK	0x170f9
			MX6SLL_PAD_SD3_DATA0__SD3_DATA0	0x170f9
			MX6SLL_PAD_SD3_DATA1__SD3_DATA1	0x170f9
			MX6SLL_PAD_SD3_DATA2__SD3_DATA2	0x170f9
			MX6SLL_PAD_SD3_DATA3__SD3_DATA3	0x170f9
		>;
	};

	pinctrl_usdhc3_sleep: usdhc3grp-sleep {
		fsl,pins = <
			MX6SLL_PAD_SD3_CMD__GPIO5_IO21	0x100c1
			MX6SLL_PAD_SD3_CLK__GPIO5_IO18	0x100c1
			MX6SLL_PAD_SD3_DATA0__GPIO5_IO19	0x100c1
			MX6SLL_PAD_SD3_DATA1__GPIO5_IO20	0x100c1
			MX6SLL_PAD_SD3_DATA2__GPIO5_IO16	0x100c1
			MX6SLL_PAD_SD3_DATA3__GPIO5_IO17	0x100c1
		>;
	};

	pinctrl_wifi_power: wifi-powergrp {
		fsl,pins = <
			MX6SLL_PAD_SD2_DATA6__GPIO4_IO29	0x10059		/* WIFI_3V3_ON */
		>;
	};

	pinctrl_wifi_reset: wifi-resetgrp {
		fsl,pins = <
			MX6SLL_PAD_SD2_DATA7__GPIO5_IO00	0x10059		/* WIFI_RST */
		>;
	};
};

&leds {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_led>;
};

&lm3630a {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_lm3630a_bl_gpio>;
};

&reg_wifi {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_wifi_power>;
};

&ricoh619 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_ricoh_gpio>;
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart1>;
};

&uart4 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart4>;
};

&usdhc2 {
	pinctrl-names = "default", "state_100mhz", "state_200mhz","sleep";
	pinctrl-0 = <&pinctrl_usdhc2>;
	pinctrl-1 = <&pinctrl_usdhc2_100mhz>;
	pinctrl-2 = <&pinctrl_usdhc2_200mhz>;
	pinctrl-3 = <&pinctrl_usdhc2_sleep>;
};

&usdhc3 {
	pinctrl-names = "default", "state_100mhz", "state_200mhz","sleep";
	pinctrl-0 = <&pinctrl_usdhc3>;
	pinctrl-1 = <&pinctrl_usdhc3_100mhz>;
	pinctrl-2 = <&pinctrl_usdhc3_200mhz>;
	pinctrl-3 = <&pinctrl_usdhc3_sleep>;
};

&wifi_pwrseq {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_wifi_reset>;
};
