// SPDX-License-Identifier: GPL-2.0-or-later
/*
 * Copyright 2013 Gateworks Corporation
 */

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/linux-event-codes.h>
#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/sound/fsl-imx-audmux.h>

/ {
	/* these are used by bootloader for disabling nodes */
	aliases {
		led0 = &led0;
		led1 = &led1;
		led2 = &led2;
		nand = &gpmi;
		ssi0 = &ssi1;
		usb0 = &usbh1;
		usb1 = &usbotg;
	};

	chosen {
		bootargs = "console=ttymxc1,115200";
	};

	backlight {
		compatible = "pwm-backlight";
		pwms = <&pwm4 0 5000000>;
		brightness-levels = <0 4 8 16 32 64 128 255>;
		default-brightness-level = <7>;
	};

	gpio-keys {
		compatible = "gpio-keys";

		user-pb {
			label = "user_pb";
			gpios = <&gsc_gpio 0 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
		};

		user-pb1x {
			label = "user_pb1x";
			linux,code = <BTN_1>;
			interrupt-parent = <&gsc>;
			interrupts = <0>;
		};

		key-erased {
			label = "key-erased";
			linux,code = <BTN_2>;
			interrupt-parent = <&gsc>;
			interrupts = <1>;
		};

		eeprom-wp {
			label = "eeprom_wp";
			linux,code = <BTN_3>;
			interrupt-parent = <&gsc>;
			interrupts = <2>;
		};

		tamper {
			label = "tamper";
			linux,code = <BTN_4>;
			interrupt-parent = <&gsc>;
			interrupts = <5>;
		};

		switch-hold {
			label = "switch_hold";
			linux,code = <BTN_5>;
			interrupt-parent = <&gsc>;
			interrupts = <7>;
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_gpio_leds>;

		led0: led-user1 {
			label = "user1";
			gpios = <&gpio4 6 GPIO_ACTIVE_HIGH>; /* MX6_PANLEDG */
			default-state = "on";
			linux,default-trigger = "heartbeat";
		};

		led1: led-user2 {
			label = "user2";
			gpios = <&gpio4 7 GPIO_ACTIVE_HIGH>; /* MX6_PANLEDR */
			default-state = "off";
		};

		led2: led-user3 {
			label = "user3";
			gpios = <&gpio4 15 GPIO_ACTIVE_LOW>; /* MX6_LOCLED# */
			default-state = "off";
		};
	};

	memory@10000000 {
		device_type = "memory";
		reg = <0x10000000 0x40000000>;
	};

	pps {
		compatible = "pps-gpio";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_pps>;
		gpios = <&gpio1 26 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};

	reg_1p0v: regulator-1p0v {
		compatible = "regulator-fixed";
		regulator-name = "1P0V";
		regulator-min-microvolt = <1000000>;
		regulator-max-microvolt = <1000000>;
		regulator-always-on;
	};

	reg_3p3v: regulator-3p3v {
		compatible = "regulator-fixed";
		regulator-name = "3P3V";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
	};

	reg_can1_stby: regulator-can1-stby {
		compatible = "regulator-fixed";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_reg_can1>;
		regulator-name = "can1_stby";
		gpio = <&gpio1 2 GPIO_ACTIVE_LOW>;
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
	};

	reg_usb_h1_vbus: regulator-usb-h1-vbus {
		compatible = "regulator-fixed";
		regulator-name = "usb_h1_vbus";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		regulator-always-on;
	};

	reg_usb_otg_vbus: regulator-usb-otg-vbus {
		compatible = "regulator-fixed";
		regulator-name = "usb_otg_vbus";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gpio3 22 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};

	sound-analog {
		compatible = "fsl,imx6q-ventana-sgtl5000",
			     "fsl,imx-audio-sgtl5000";
		model = "sgtl5000-audio";
		ssi-controller = <&ssi1>;
		audio-codec = <&sgtl5000>;
		audio-routing =
			"MIC_IN", "Mic Jack",
			"Mic Jack", "Mic Bias",
			"Headphone Jack", "HP_OUT";
		mux-int-port = <1>;
		mux-ext-port = <4>;
	};
};

&audmux {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_audmux>; /* AUD4<->sgtl5000 */
	status = "okay";

	mux-ssi2 {
		fsl,audmux-port = <1>;
		fsl,port-config = <
			(IMX_AUDMUX_V2_PTCR_TFSDIR |
			IMX_AUDMUX_V2_PTCR_TFSEL(4+8) | /* RXFS */
			IMX_AUDMUX_V2_PTCR_TCLKDIR |
			IMX_AUDMUX_V2_PTCR_TCSEL(4+8) | /* RXC */
			IMX_AUDMUX_V2_PTCR_SYN)
			IMX_AUDMUX_V2_PDCR_RXDSEL(4)
		>;
	};

	mux-aud5 {
		fsl,audmux-port = <4>;
		fsl,port-config = <
			IMX_AUDMUX_V2_PTCR_SYN
			IMX_AUDMUX_V2_PDCR_RXDSEL(1)>;
	};
};

&can1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_flexcan1>;
	xceiver-supply = <&reg_can1_stby>;
	status = "okay";
};

&clks {
	assigned-clocks = <&clks IMX6QDL_CLK_LDB_DI0_SEL>,
			  <&clks IMX6QDL_CLK_LDB_DI1_SEL>;
	assigned-clock-parents = <&clks IMX6QDL_CLK_PLL3_USB_OTG>,
				 <&clks IMX6QDL_CLK_PLL3_USB_OTG>;
};

&ecspi2 {
	cs-gpios = <&gpio2 26 GPIO_ACTIVE_LOW>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_ecspi2>;
	status = "okay";
};

&fec {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_enet>;
	phy-mode = "rgmii-id";
	phy-reset-gpios = <&gpio1 30 GPIO_ACTIVE_LOW>;
	status = "okay";
};

&gpmi {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_gpmi_nand>;
	status = "okay";
};

&hdmi {
	ddc-i2c-bus = <&i2c3>;
	status = "okay";
};

&i2c1 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c1>;
	status = "okay";

	gsc: gsc@20 {
		compatible = "gw,gsc";
		reg = <0x20>;
		interrupt-parent = <&gpio1>;
		interrupts = <4 IRQ_TYPE_LEVEL_LOW>;
		interrupt-controller;
		#interrupt-cells = <1>;
		#address-cells = <1>;
		#size-cells = <0>;

		adc {
			compatible = "gw,gsc-adc";
			#address-cells = <1>;
			#size-cells = <0>;

			channel@0 {
				gw,mode = <0>;
				reg = <0x00>;
				label = "temp";
			};

			channel@2 {
				gw,mode = <1>;
				reg = <0x02>;
				label = "vdd_vin";
			};

			channel@5 {
				gw,mode = <1>;
				reg = <0x05>;
				label = "vdd_3p3";
			};

			channel@8 {
				gw,mode = <1>;
				reg = <0x08>;
				label = "vdd_bat";
			};

			channel@b {
				gw,mode = <1>;
				reg = <0x0b>;
				label = "vdd_5p0";
			};

			channel@e {
				gw,mode = <1>;
				reg = <0xe>;
				label = "vdd_arm";
			};

			channel@11 {
				gw,mode = <1>;
				reg = <0x11>;
				label = "vdd_soc";
			};

			channel@14 {
				gw,mode = <1>;
				reg = <0x14>;
				label = "vdd_3p0";
			};

			channel@17 {
				gw,mode = <1>;
				reg = <0x17>;
				label = "vdd_1p5";
			};

			channel@1d {
				gw,mode = <1>;
				reg = <0x1d>;
				label = "vdd_1p8";
			};

			channel@20 {
				gw,mode = <1>;
				reg = <0x20>;
				label = "vdd_1p0";
			};

			channel@23 {
				gw,mode = <1>;
				reg = <0x23>;
				label = "vdd_2p5";
			};

			channel@26 {
				gw,mode = <1>;
				reg = <0x26>;
				label = "vdd_gps";
			};
		};

		fan-controller@2c {
			compatible = "gw,gsc-fan";
			reg = <0x2c>;
		};
	};

	gsc_gpio: gpio@23 {
		compatible = "nxp,pca9555";
		reg = <0x23>;
		gpio-controller;
		#gpio-cells = <2>;
		interrupt-parent = <&gsc>;
		interrupts = <4>;
	};

	eeprom1: eeprom@50 {
		compatible = "atmel,24c02";
		reg = <0x50>;
		pagesize = <16>;
	};

	eeprom2: eeprom@51 {
		compatible = "atmel,24c02";
		reg = <0x51>;
		pagesize = <16>;
	};

	eeprom3: eeprom@52 {
		compatible = "atmel,24c02";
		reg = <0x52>;
		pagesize = <16>;
	};

	eeprom4: eeprom@53 {
		compatible = "atmel,24c02";
		reg = <0x53>;
		pagesize = <16>;
	};

	rtc: ds1672@68 {
		compatible = "dallas,ds1672";
		reg = <0x68>;
	};
};

&i2c2 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c2>;
	status = "okay";

	pmic: pmic@8 {
		compatible = "fsl,pfuze100";
		reg = <0x08>;

		regulators {
			sw1a_reg: sw1ab {
				regulator-min-microvolt = <300000>;
				regulator-max-microvolt = <1875000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-ramp-delay = <6250>;
			};

			sw1c_reg: sw1c {
				regulator-min-microvolt = <300000>;
				regulator-max-microvolt = <1875000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-ramp-delay = <6250>;
			};

			sw2_reg: sw2 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <3950000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw3a_reg: sw3a {
				regulator-min-microvolt = <400000>;
				regulator-max-microvolt = <1975000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw3b_reg: sw3b {
				regulator-min-microvolt = <400000>;
				regulator-max-microvolt = <1975000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw4_reg: sw4 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <3300000>;
			};

			swbst_reg: swbst {
				regulator-min-microvolt = <5000000>;
				regulator-max-microvolt = <5150000>;
				regulator-boot-on;
				regulator-always-on;
			};

			snvs_reg: vsnvs {
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <3000000>;
				regulator-boot-on;
				regulator-always-on;
			};

			vref_reg: vrefddr {
				regulator-boot-on;
				regulator-always-on;
			};

			vgen1_reg: vgen1 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1550000>;
			};

			vgen2_reg: vgen2 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1550000>;
			};

			vgen3_reg: vgen3 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
			};

			vgen4_reg: vgen4 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen5_reg: vgen5 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen6_reg: vgen6 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};
		};
	};
};

&i2c3 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c3>;
	status = "okay";

	sgtl5000: audio-codec@a {
		compatible = "fsl,sgtl5000";
		reg = <0x0a>;
		#sound-dai-cells = <0>;
		clocks = <&clks IMX6QDL_CLK_CKO>;
		VDDA-supply = <&sw4_reg>;
		VDDIO-supply = <&reg_3p3v>;
	};

	touchscreen: egalax_ts@4 {
		compatible = "eeti,egalax_ts";
		reg = <0x04>;
		interrupt-parent = <&gpio7>;
		interrupts = <12 2>;
		wakeup-gpios = <&gpio7 12 GPIO_ACTIVE_LOW>;
	};

	accel@1e {
		compatible = "nxp,fxos8700";
		reg = <0x1e>;
	};
};

&ldb {
	status = "okay";

	lvds-channel@0 {
		fsl,data-mapping = "spwg";
		fsl,data-width = <18>;
		status = "okay";

		display-timings {
			native-mode = <&timing0>;
			timing0: hsd100pxn1 {
				clock-frequency = <65000000>;
				hactive = <1024>;
				vactive = <768>;
				hback-porch = <220>;
				hfront-porch = <40>;
				vback-porch = <21>;
				vfront-porch = <7>;
				hsync-len = <60>;
				vsync-len = <10>;
			};
		};
	};
};

&pcie {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_pcie>;
	reset-gpio = <&gpio1 29 GPIO_ACTIVE_LOW>;
	status = "okay";
};

&pwm1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_pwm1>; /* MX6_DIO0 */
	status = "disabled";
};

&pwm2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_pwm2>; /* MX6_DIO1 */
	status = "disabled";
};

&pwm3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_pwm3>; /* MX6_DIO2 */
	status = "disabled";
};

&pwm4 {
	#pwm-cells = <2>;
	pinctrl-names = "default", "state_dio";
	pinctrl-0 = <&pinctrl_pwm4_backlight>;
	pinctrl-1 = <&pinctrl_pwm4_dio>;
	status = "okay";
};

&ssi1 {
	status = "okay";
};

&ssi2 {
	status = "okay";
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart1>;
	rts-gpios = <&gpio7 1 GPIO_ACTIVE_HIGH>;
	status = "okay";
};

&uart2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart2>;
	status = "okay";
};

&uart5 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart5>;
	status = "okay";
};

&usbotg {
	vbus-supply = <&reg_usb_otg_vbus>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usbotg>;
	disable-over-current;
	status = "okay";
};

&usbh1 {
	vbus-supply = <&reg_usb_h1_vbus>;
	status = "okay";
};

&usdhc3 {
	pinctrl-names = "default", "state_100mhz", "state_200mhz";
	pinctrl-0 = <&pinctrl_usdhc3>;
	pinctrl-1 = <&pinctrl_usdhc3_100mhz>;
	pinctrl-2 = <&pinctrl_usdhc3_200mhz>;
	cd-gpios = <&gpio7 0 GPIO_ACTIVE_LOW>;
	vmmc-supply = <&reg_3p3v>;
	no-1-8-v; /* firmware will remove if board revision supports */
	status = "okay";
};

&wdog1 {
	status = "disabled";
};

&wdog2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_wdog>;
	fsl,ext-reset-output;
	status = "okay";
};

&iomuxc {
	pinctrl_audmux: audmuxgrp {
		fsl,pins = <
			MX6QDL_PAD_SD2_DAT0__AUD4_RXD		0x130b0
			MX6QDL_PAD_SD2_DAT3__AUD4_TXC		0x130b0
			MX6QDL_PAD_SD2_DAT2__AUD4_TXD		0x110b0
			MX6QDL_PAD_SD2_DAT1__AUD4_TXFS		0x130b0
			MX6QDL_PAD_GPIO_0__CCM_CLKO1		0x130b0 /* AUD4_MCK */
			MX6QDL_PAD_EIM_D25__AUD5_RXC            0x130b0
			MX6QDL_PAD_DISP0_DAT19__AUD5_RXD        0x130b0
			MX6QDL_PAD_EIM_D24__AUD5_RXFS           0x130b0
		>;
	};

	pinctrl_enet: enetgrp {
		fsl,pins = <
			MX6QDL_PAD_RGMII_RXC__RGMII_RXC		0x1b030
			MX6QDL_PAD_RGMII_RD0__RGMII_RD0		0x1b030
			MX6QDL_PAD_RGMII_RD1__RGMII_RD1		0x1b030
			MX6QDL_PAD_RGMII_RD2__RGMII_RD2		0x1b030
			MX6QDL_PAD_RGMII_RD3__RGMII_RD3		0x1b030
			MX6QDL_PAD_RGMII_RX_CTL__RGMII_RX_CTL	0x1b030
			MX6QDL_PAD_RGMII_TXC__RGMII_TXC		0x1b030
			MX6QDL_PAD_RGMII_TD0__RGMII_TD0		0x1b030
			MX6QDL_PAD_RGMII_TD1__RGMII_TD1		0x1b030
			MX6QDL_PAD_RGMII_TD2__RGMII_TD2		0x1b030
			MX6QDL_PAD_RGMII_TD3__RGMII_TD3		0x1b030
			MX6QDL_PAD_RGMII_TX_CTL__RGMII_TX_CTL	0x1b030
			MX6QDL_PAD_ENET_REF_CLK__ENET_TX_CLK	0x1b0b0
			MX6QDL_PAD_ENET_MDIO__ENET_MDIO		0x1b0b0
			MX6QDL_PAD_ENET_MDC__ENET_MDC		0x1b0b0
			MX6QDL_PAD_GPIO_16__ENET_REF_CLK	0x4001b0a8
		>;
	};

	pinctrl_ecspi2: escpi2grp {
		fsl,pins = <
			MX6QDL_PAD_EIM_CS0__ECSPI2_SCLK	0x100b1
			MX6QDL_PAD_EIM_CS1__ECSPI2_MOSI	0x100b1
			MX6QDL_PAD_EIM_OE__ECSPI2_MISO	0x100b1
			MX6QDL_PAD_EIM_RW__GPIO2_IO26	0x100b1
		>;
	};

	pinctrl_flexcan1: flexcan1grp {
		fsl,pins = <
			MX6QDL_PAD_KEY_ROW2__FLEXCAN1_RX	0x1b0b1
			MX6QDL_PAD_KEY_COL2__FLEXCAN1_TX	0x1b0b1
		>;
	};

	pinctrl_gpio_leds: gpioledsgrp {
		fsl,pins = <
			MX6QDL_PAD_KEY_COL0__GPIO4_IO06		0x1b0b0
			MX6QDL_PAD_KEY_ROW0__GPIO4_IO07		0x1b0b0
			MX6QDL_PAD_KEY_ROW4__GPIO4_IO15		0x1b0b0
		>;
	};

	pinctrl_gpmi_nand: gpminandgrp {
		fsl,pins = <
			MX6QDL_PAD_NANDF_CLE__NAND_CLE		0xb0b1
			MX6QDL_PAD_NANDF_ALE__NAND_ALE		0xb0b1
			MX6QDL_PAD_NANDF_WP_B__NAND_WP_B	0xb0b1
			MX6QDL_PAD_NANDF_RB0__NAND_READY_B	0xb000
			MX6QDL_PAD_NANDF_CS0__NAND_CE0_B	0xb0b1
			MX6QDL_PAD_SD4_CMD__NAND_RE_B		0xb0b1
			MX6QDL_PAD_SD4_CLK__NAND_WE_B		0xb0b1
			MX6QDL_PAD_NANDF_D0__NAND_DATA00	0xb0b1
			MX6QDL_PAD_NANDF_D1__NAND_DATA01	0xb0b1
			MX6QDL_PAD_NANDF_D2__NAND_DATA02	0xb0b1
			MX6QDL_PAD_NANDF_D3__NAND_DATA03	0xb0b1
			MX6QDL_PAD_NANDF_D4__NAND_DATA04	0xb0b1
			MX6QDL_PAD_NANDF_D5__NAND_DATA05	0xb0b1
			MX6QDL_PAD_NANDF_D6__NAND_DATA06	0xb0b1
			MX6QDL_PAD_NANDF_D7__NAND_DATA07	0xb0b1
		>;
	};

	pinctrl_i2c1: i2c1grp {
		fsl,pins = <
			MX6QDL_PAD_EIM_D21__I2C1_SCL		0x4001b8b1
			MX6QDL_PAD_EIM_D28__I2C1_SDA		0x4001b8b1
			MX6QDL_PAD_GPIO_4__GPIO1_IO04		0xb0b1
		>;
	};

	pinctrl_i2c2: i2c2grp {
		fsl,pins = <
			MX6QDL_PAD_KEY_COL3__I2C2_SCL		0x4001b8b1
			MX6QDL_PAD_KEY_ROW3__I2C2_SDA		0x4001b8b1
		>;
	};

	pinctrl_i2c3: i2c3grp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_3__I2C3_SCL		0x4001b8b1
			MX6QDL_PAD_GPIO_6__I2C3_SDA		0x4001b8b1
		>;
	};

	pinctrl_pcie: pciegrp {
		fsl,pins = <
			MX6QDL_PAD_ENET_TX_EN__GPIO1_IO28	0x1b0b0 /* PCIE IRQ */
			MX6QDL_PAD_ENET_TXD1__GPIO1_IO29	0x1b0b0 /* PCIE RST */
		>;
	};

	pinctrl_pps: ppsgrp {
		fsl,pins = <
			MX6QDL_PAD_ENET_RXD1__GPIO1_IO26	0x1b0b1
		>;
	};

	pinctrl_pwm1: pwm1grp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_9__PWM1_OUT		0x1b0b1
		>;
	};

	pinctrl_pwm2: pwm2grp {
		fsl,pins = <
			MX6QDL_PAD_SD1_DAT2__PWM2_OUT		0x1b0b1
		>;
	};

	pinctrl_pwm3: pwm3grp {
		fsl,pins = <
			MX6QDL_PAD_SD4_DAT1__PWM3_OUT		0x1b0b1
		>;
	};

	pinctrl_pwm4_backlight: pwm4grpbacklight {
		fsl,pins = <
			/* LVDS_PWM J6.5 */
			MX6QDL_PAD_SD1_CMD__PWM4_OUT		0x1b0b1
		>;
	};

	pinctrl_pwm4_dio: pwm4grpdio {
		fsl,pins = <
			/* DIO3 J16.4 */
			MX6QDL_PAD_SD4_DAT2__PWM4_OUT		0x1b0b1
		>;
	};

	pinctrl_reg_can1: regcan1grp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_2__GPIO1_IO02		0x4001b0b0 /* CAN_STBY */
		>;
	};

	pinctrl_uart1: uart1grp {
		fsl,pins = <
			MX6QDL_PAD_SD3_DAT7__UART1_TX_DATA	0x1b0b1
			MX6QDL_PAD_SD3_DAT6__UART1_RX_DATA	0x1b0b1
			MX6QDL_PAD_SD3_DAT4__GPIO7_IO01		0x4001b0b1 /* TEN */
		>;
	};

	pinctrl_uart2: uart2grp {
		fsl,pins = <
			MX6QDL_PAD_SD4_DAT7__UART2_TX_DATA	0x1b0b1
			MX6QDL_PAD_SD4_DAT4__UART2_RX_DATA	0x1b0b1
		>;
	};

	pinctrl_uart5: uart5grp {
		fsl,pins = <
			MX6QDL_PAD_KEY_COL1__UART5_TX_DATA	0x1b0b1
			MX6QDL_PAD_KEY_ROW1__UART5_RX_DATA	0x1b0b1
		>;
	};

	pinctrl_usbotg: usbotggrp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_1__USB_OTG_ID		0x17059
			MX6QDL_PAD_EIM_D22__GPIO3_IO22		0x1b0b0 /* PWR_EN */
			MX6QDL_PAD_KEY_COL4__USB_OTG_OC		0x17059
		>;
	};

	pinctrl_usdhc3: usdhc3grp {
		fsl,pins = <
			MX6QDL_PAD_SD3_CMD__SD3_CMD		0x17059
			MX6QDL_PAD_SD3_CLK__SD3_CLK		0x10059
			MX6QDL_PAD_SD3_DAT0__SD3_DATA0		0x17059
			MX6QDL_PAD_SD3_DAT1__SD3_DATA1		0x17059
			MX6QDL_PAD_SD3_DAT2__SD3_DATA2		0x17059
			MX6QDL_PAD_SD3_DAT3__SD3_DATA3		0x17059
			MX6QDL_PAD_SD3_DAT5__GPIO7_IO00		0x17059 /* CD */
			MX6QDL_PAD_NANDF_CS1__SD3_VSELECT	0x17059
		>;
	};

	pinctrl_usdhc3_100mhz: usdhc3grp100mhz {
		fsl,pins = <
			MX6QDL_PAD_SD3_CMD__SD3_CMD		0x170b9
			MX6QDL_PAD_SD3_CLK__SD3_CLK		0x100b9
			MX6QDL_PAD_SD3_DAT0__SD3_DATA0		0x170b9
			MX6QDL_PAD_SD3_DAT1__SD3_DATA1		0x170b9
			MX6QDL_PAD_SD3_DAT2__SD3_DATA2		0x170b9
			MX6QDL_PAD_SD3_DAT3__SD3_DATA3		0x170b9
			MX6QDL_PAD_SD3_DAT5__GPIO7_IO00		0x170b9 /* CD */
			MX6QDL_PAD_NANDF_CS1__SD3_VSELECT	0x170b9
		>;
	};

	pinctrl_usdhc3_200mhz: usdhc3grp200mhz {
		fsl,pins = <
			MX6QDL_PAD_SD3_CMD__SD3_CMD		0x170f9
			MX6QDL_PAD_SD3_CLK__SD3_CLK		0x100f9
			MX6QDL_PAD_SD3_DAT0__SD3_DATA0		0x170f9
			MX6QDL_PAD_SD3_DAT1__SD3_DATA1		0x170f9
			MX6QDL_PAD_SD3_DAT2__SD3_DATA2		0x170f9
			MX6QDL_PAD_SD3_DAT3__SD3_DATA3		0x170f9
			MX6QDL_PAD_SD3_DAT5__GPIO7_IO00		0x170f9 /* CD */
			MX6QDL_PAD_NANDF_CS1__SD3_VSELECT	0x170f9
		>;
	};

	pinctrl_wdog: wdoggrp {
		fsl,pins = <
			MX6QDL_PAD_SD1_DAT3__WDOG2_B		0x1b0b0
		>;
	};
};
