// SPDX-License-Identifier: (GPL-2.0 OR MIT)
/*
 * Copyright (C) 2016-2017 Zodiac Inflight Innovations
 */

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/sound/fsl-imx-audmux.h>

/ {
	chosen {
		stdout-path = &uart1;
	};

	aliases {
		mdio-gpio0 = &mdio1;
		rtc0 = &ds1341;
	};

	mdio1: mdio {
		compatible = "virtual,mdio-gpio";
		#address-cells = <1>;
		#size-cells = <0>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_mdio1>;
		gpios = <&gpio6 5 GPIO_ACTIVE_HIGH
		         &gpio6 4 GPIO_ACTIVE_HIGH>;

		phy: ethernet-phy@0 {
			pinctrl-0 = <&pinctrl_rmii_phy_irq>;
			pinctrl-names = "default";
			reg = <0>;
			interrupt-parent = <&gpio3>;
			interrupts = <30 IRQ_TYPE_LEVEL_LOW>;
		};
	};

	reg_28p0v: regulator-28p0v {
		compatible = "regulator-fixed";
		regulator-name = "28V_IN";
		regulator-min-microvolt = <28000000>;
		regulator-max-microvolt = <28000000>;
		regulator-always-on;
	};

	reg_12p0v: regulator-12p0v {
		compatible = "regulator-fixed";
		vin-supply = <&reg_28p0v>;
		regulator-name = "12V_MAIN";
		regulator-min-microvolt = <12000000>;
		regulator-max-microvolt = <12000000>;
		regulator-always-on;
	};

	reg_5p0v_main: regulator-5p0v-main {
		compatible = "regulator-fixed";
		vin-supply = <&reg_12p0v>;
		regulator-name = "5V_MAIN";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		regulator-always-on;
	};

	reg_3p3v_pmic: regulator-3p3v-pmic {
		compatible = "regulator-fixed";
		vin-supply = <&reg_12p0v>;
		regulator-name = "PMIC_3V3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
	};

	reg_3p3v: regulator-3p3v {
		compatible = "regulator-fixed";
		vin-supply = <&reg_3p3v_pmic>;
		regulator-name = "GEN_3V3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
	};

	reg_3p3v_sd: regulator-3p3v-sd {
		compatible = "regulator-fixed";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_reg_3p3v_sd>;
		vin-supply = <&reg_3p3v>;
		regulator-name = "3V3_SD";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		gpio = <&gpio7 8 GPIO_ACTIVE_HIGH>;
		startup-delay-us = <1000>;
		enable-active-high;
		regulator-always-on;
	};

	reg_3p3v_display: regulator-3p3v-display {
		compatible = "regulator-fixed";
		vin-supply = <&reg_12p0v>;
		regulator-name = "3V3_DISPLAY";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
	};

	reg_3p3v_ssd: regulator-3p3v-ssd {
		compatible = "regulator-fixed";
		vin-supply = <&reg_12p0v>;
		regulator-name = "3V3_SSD";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
	};

	sound1 {
		compatible = "simple-audio-card";
		simple-audio-card,name = "front";
		simple-audio-card,format = "i2s";
		simple-audio-card,bitclock-master = <&sound1_codec>;
		simple-audio-card,frame-master = <&sound1_codec>;
		simple-audio-card,widgets =
			"Headphone", "Headphone Jack";
		simple-audio-card,routing =
			"Headphone Jack", "HPA1 HPLEFT",
			"Headphone Jack", "HPA1 HPRIGHT",
			"HPA1 LEFTIN", "HPL",
			"HPA1 RIGHTIN", "HPR";
		simple-audio-card,aux-devs = <&hpa1>;

		sound1_cpu: simple-audio-card,cpu {
			sound-dai = <&ssi2>;
		};

		sound1_codec: simple-audio-card,codec {
			sound-dai = <&codec1>;
			clocks = <&cs2000>;
		};
	};

	sound2 {
		compatible = "simple-audio-card";
		simple-audio-card,name = "periph";
		simple-audio-card,format = "i2s";
		simple-audio-card,bitclock-master = <&sound2_codec>;
		simple-audio-card,frame-master = <&sound2_codec>;
		simple-audio-card,widgets =
			"Headphone", "Headphone Jack";
		simple-audio-card,routing =
			"Headphone Jack", "HPA1 HPLEFT",
			"Headphone Jack", "HPA1 HPRIGHT",
			"HPA1 LEFTIN", "HPL",
			"HPA1 RIGHTIN", "HPR";
		simple-audio-card,aux-devs = <&hpa2>;

		sound2_cpu: simple-audio-card,cpu {
			sound-dai = <&ssi1>;
		};

		sound2_codec: simple-audio-card,codec {
			sound-dai = <&codec2>;
			clocks = <&cs2000>;
		};
	};

	panel {
		power-supply = <&reg_3p3v_display>;
		backlight = <&sp_backlight>;
		status = "disabled";

		port {
			panel_in: endpoint {
				remote-endpoint = <&lvds0_out>;
			};
		};
	};

	disp0: disp0 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "fsl,imx-parallel-display";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_disp0>;
		status = "disabled";

		port@0 {
			reg = <0>;

			disp0_in_0: endpoint {
				remote-endpoint = <&ipu1_di0_disp0>;
			};
		};

		port@1 {
			reg = <1>;

			disp0_out: endpoint {
				remote-endpoint = <&tc358767_in>;
			};
		};
	};

	cs2000_ref: cs2000-ref {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <24576000>;
	};

	cs2000_in_dummy: cs2000-in-dummy {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <0>;
	};

	edp_refclk: edp-refclk {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <19200000>;
	};
};

&clks {
	assigned-clocks = <&clks IMX6QDL_CLK_LDB_DI0_SEL>,
	                  <&clks IMX6QDL_CLK_LDB_DI1_SEL>;
	assigned-clock-parents = <&clks IMX6QDL_CLK_PLL5_VIDEO_DIV>,
	                         <&clks IMX6QDL_CLK_PLL5_VIDEO_DIV>;
};

&cpu0 {
	fsl,soc-operating-points = <
		/* ARM kHz  SOC-PU uV */
		1200000 1300000
		996000	1275000
		852000	1275000
		792000	1200000
		396000	1200000
	>;
};

&reg_arm {
	vin-supply = <&sw1a_reg>;
};

&reg_pu {
	vin-supply = <&sw1c_reg>;
};

&reg_soc {
	vin-supply = <&sw1c_reg>;
};

&ldb {
	lvds-channel@0 {
		port@4 {
			reg = <4>;

			lvds0_out: endpoint {
				remote-endpoint = <&panel_in>;
			};
		};
	};
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart1>;
	status = "okay";
};

&uart3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart3>;
	uart-has-rtscts;
	linux,rs485-enabled-at-boot-time;
	status = "okay";
};

&uart4 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart4>;
	status = "okay";

	mcu {
		compatible = "zii,rave-sp-rdu2";
		current-speed = <1000000>;
		#address-cells = <1>;
		#size-cells = <1>;

		watchdog {
			compatible = "zii,rave-sp-watchdog";
		};

		sp_backlight: backlight {
			compatible = "zii,rave-sp-backlight";
		};

		pwrbutton {
			compatible = "zii,rave-sp-pwrbutton";
		};

		eeprom@a3 {
			compatible = "zii,rave-sp-eeprom";
			reg = <0xa3 0x4000>;
			#address-cells = <1>;
			#size-cells = <1>;
			zii,eeprom-name = "dds-eeprom";
		};

		eeprom@a4 {
			compatible = "zii,rave-sp-eeprom";
			reg = <0xa4 0x4000>;
			#address-cells = <1>;
			#size-cells = <1>;
			zii,eeprom-name = "main-eeprom";
		};
	};
};

&ecspi1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_ecspi1>;
	cs-gpios = <&gpio2 30 GPIO_ACTIVE_LOW>;
	status = "okay";

	flash@0 {
		compatible = "st,m25p128", "jedec,spi-nor";
		spi-max-frequency = <20000000>;
		reg = <0>;
	};
};

&gpio3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_gpio3_hog>;

	usb-emulation-hog {
		gpio-hog;
		gpios = <19 GPIO_ACTIVE_HIGH>;
		output-low;
		line-name = "usb-emulation";
	};

	usb-mode1-hog {
		gpio-hog;
		gpios = <20 GPIO_ACTIVE_HIGH>;
		output-high;
		line-name = "usb-mode1";
	};

	usb-pwr-hog {
		gpio-hog;
		gpios = <22 GPIO_ACTIVE_LOW>;
		output-high;
		line-name = "usb-pwr-ctrl-en-n";
	};

	usb-mode2-hog {
		gpio-hog;
		gpios = <23 GPIO_ACTIVE_HIGH>;
		output-high;
		line-name = "usb-mode2";
	};
};

&i2c1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c1>;
	clock-frequency = <100000>;
	status = "okay";

	codec2: codec@18 {
		compatible = "ti,tlv320dac3100";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_codec2>;
		reg = <0x18>;
		#sound-dai-cells = <0>;
		HPVDD-supply = <&reg_3p3v>;
		SPRVDD-supply = <&reg_3p3v>;
		SPLVDD-supply = <&reg_3p3v>;
		AVDD-supply = <&reg_3p3v>;
		IOVDD-supply = <&reg_3p3v>;
		DVDD-supply = <&vgen4_reg>;
		reset-gpios = <&gpio1 2 GPIO_ACTIVE_LOW>;
	};

	accel@1c {
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_accel>;
		compatible = "fsl,mma8451";
		reg = <0x1c>;
		interrupt-parent = <&gpio1>;
		interrupt-names = "INT2";
		interrupts = <20 IRQ_TYPE_LEVEL_LOW>;
		vdd-supply = <&reg_3p3v>;
		vddio-supply = <&reg_3p3v>;
	};

	hpa2: amp@60 {
		compatible = "ti,tpa6130a2";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_tpa2>;
		reg = <0x60>;
		power-gpio = <&gpio1 5 GPIO_ACTIVE_HIGH>;
		Vdd-supply = <&reg_5p0v_main>;
		sound-name-prefix = "HPA1";
	};

	edp-bridge@68 {
		compatible = "toshiba,tc358767";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_tc358767>;
		reg = <0x68>;
		shutdown-gpios = <&gpio1 9 GPIO_ACTIVE_HIGH>;
		clock-names = "ref";
		clocks = <&edp_refclk>;
		status = "disabled";

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@1 {
				reg = <1>;

				tc358767_in: endpoint {
					remote-endpoint = <&disp0_out>;
				};
			};
		};
	};
};

&i2c2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c2>;
	clock-frequency = <100000>;
	status = "okay";

	pmic@8 {
		compatible = "fsl,pfuze100";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_pfuze100_irq>;
		reg = <0x08>;
		interrupt-parent = <&gpio7>;
		interrupts = <13 IRQ_TYPE_LEVEL_LOW>;

		regulators {
			sw1a_reg: sw1ab {
				regulator-min-microvolt = <300000>;
				regulator-max-microvolt = <1875000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-ramp-delay = <6250>;
			};

			sw1c_reg: sw1c {
				regulator-min-microvolt = <300000>;
				regulator-max-microvolt = <1875000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-ramp-delay = <6250>;
			};

			sw2_reg: sw2 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <3000000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw3a_reg: sw3a {
				regulator-min-microvolt = <400000>;
				regulator-max-microvolt = <1500000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw3b_reg: sw3b {
				regulator-min-microvolt = <400000>;
				regulator-max-microvolt = <1500000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw4_reg: sw4 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1800000>;
				regulator-boot-on;
				regulator-always-on;
			};

			snvs_reg: vsnvs {
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <3000000>;
				regulator-boot-on;
				regulator-always-on;
			};

			vref_reg: vrefddr {
				regulator-boot-on;
				regulator-always-on;
			};

			vgen2_reg: vgen2 {
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1500000>;
				regulator-always-on;
			};

			vgen4_reg: vgen4 {
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <1800000>;
				regulator-always-on;
			};

			vgen5_reg: vgen5 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <2500000>;
				regulator-always-on;
			};

			vgen6_reg: vgen6 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <2800000>;
				regulator-always-on;
			};
		};
	};

	watchdog@38 {
		compatible = "zii,rave-wdt";
		reg = <0x38>;
	};

	temp-sense@48 {
		compatible = "national,lm75";
		reg = <0x48>;
	};

	cs2000: clkgen@4e {
		compatible = "cirrus,cs2000-cp";
		reg = <0x4e>;
		#clock-cells = <0>;
		clock-names = "clk_in", "ref_clk";
		clocks = <&cs2000_in_dummy>, <&cs2000_ref>;
		assigned-clocks = <&cs2000>;
		assigned-clock-rates = <24000000>;
	};

	eeprom@54 {
		compatible = "atmel,24c128";
		reg = <0x54>;
	};

	ds1341: rtc@68 {
		compatible = "dallas,ds1341";
		reg = <0x68>;
	};
};

&i2c3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c3>;
	clock-frequency = <400000>;
	status = "okay";

	codec1: codec@18 {
		compatible = "ti,tlv320dac3100";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_codec1>;
		reg = <0x18>;
		#sound-dai-cells = <0>;
		HPVDD-supply = <&reg_3p3v>;
		SPRVDD-supply = <&reg_3p3v>;
		SPLVDD-supply = <&reg_3p3v>;
		AVDD-supply = <&reg_3p3v>;
		IOVDD-supply = <&reg_3p3v>;
		DVDD-supply = <&vgen4_reg>;
		reset-gpios = <&gpio1 0 GPIO_ACTIVE_LOW>;
	};

	touchscreen@20 {
		compatible = "syna,rmi4-i2c";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_ts>;
		reg = <0x20>;
		interrupt-parent = <&gpio1>;
		interrupts = <8 IRQ_TYPE_LEVEL_LOW>;
		vdd-supply = <&reg_5p0v_main>;
		vio-supply = <&reg_3p3v>;

		#address-cells = <1>;
		#size-cells = <0>;

		rmi4-f01@1 {
			reg = <0x1>;
			syna,nosleep-mode = <2>;
		};

		rmi4-f11@11 {
			reg = <0x11>;
			touchscreen-inverted-x;
			touchscreen-swapped-x-y;
			syna,sensor-type = <1>;
			syna,delta-x-threshold = <5>;
			syna,delta-y-threshold = <10>;
		};

		rmi4-f12@12 {
			reg = <0x12>;
			touchscreen-inverted-x;
			touchscreen-swapped-x-y;
			syna,sensor-type = <1>;
		};
	};

	touchscreen@2a {
		compatible = "eeti,exc3000";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_ts>;
		reg = <0x2a>;
		interrupt-parent = <&gpio1>;
		interrupts = <8 IRQ_TYPE_LEVEL_LOW>;
		touchscreen-inverted-x;
		touchscreen-swapped-x-y;
		status = "disabled";
	};

	reg_5p0v_user_usb: charger@32 {
		compatible = "microchip,ucs1002";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_ucs1002_pins>;
		reg = <0x32>;
		interrupts-extended = <&gpio5 2 IRQ_TYPE_EDGE_BOTH>,
		                      <&gpio3 21 IRQ_TYPE_EDGE_FALLING>;
		interrupt-names = "a_det", "alert";
	};

	hpa1: amp@60 {
		compatible = "ti,tpa6130a2";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_tpa1>;
		reg = <0x60>;
		power-gpio = <&gpio1 4 GPIO_ACTIVE_HIGH>;
		Vdd-supply = <&reg_5p0v_main>;
		sound-name-prefix = "HPA1";
	};
};

&ipu1_di0_disp0 {
	remote-endpoint = <&disp0_in_0>;
};

&pcie {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_pcie>;
	reset-gpio = <&gpio7 12 GPIO_ACTIVE_LOW>;
	status = "okay";

	host@0 {
		reg = <0 0 0 0 0>;

		#address-cells = <3>;
		#size-cells = <2>;

		i210: i210@0 {
			reg = <0 0 0 0 0>;
		};
	};
};

&usdhc2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc2>;
	bus-width = <4>;
	cd-gpios = <&gpio2 2 GPIO_ACTIVE_LOW>;
	disable-wp;
	vmmc-supply = <&reg_3p3v_sd>;
	vqmmc-supply = <&reg_3p3v>;
	no-1-8-v;
	no-sdio;
	status = "okay";
};

&usdhc3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc3>;
	bus-width = <4>;
	cd-gpios = <&gpio2 0 GPIO_ACTIVE_LOW>;
	disable-wp;
	vmmc-supply = <&reg_3p3v_sd>;
	vqmmc-supply = <&reg_3p3v>;
	no-1-8-v;
	no-sdio;
	status = "okay";
};

&usdhc4 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc4>;
	bus-width = <8>;
	vmmc-supply = <&reg_3p3v>;
	vqmmc-supply = <&reg_3p3v>;
	no-1-8-v;
	non-removable;
	no-sdio;
	no-sd;
	status = "okay";
};

&sata {
	target-supply = <&reg_3p3v_ssd>;
	status = "okay";
};

&fec {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_enet>;
	phy-mode = "rmii";
	phy-handle = <&phy>;
	phy-reset-gpios = <&gpio1 23 GPIO_ACTIVE_LOW>;
	phy-reset-duration = <100>;
	phy-supply = <&reg_3p3v>;
	status = "okay";

	mdio {
		#address-cells = <1>;
		#size-cells = <0>;
		clock-frequency = <12500000>;
		suppress-preamble;
		status = "okay";

		switch: switch@0 {
			compatible = "marvell,mv88e6085";
			pinctrl-0 = <&pinctrl_switch_irq>;
			pinctrl-names = "default";
			reg = <0>;
			dsa,member = <0 0>;
			eeprom-length = <512>;
			interrupt-parent = <&gpio6>;
			interrupts = <3 IRQ_TYPE_LEVEL_LOW>;
			interrupt-controller;
			#interrupt-cells = <2>;

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;
					label = "gigabit_proc";
					phy-handle = <&switchphy0>;
				};

				port@1 {
					reg = <1>;
					label = "netaux";
					phy-handle = <&switchphy1>;
				};

				port@2 {
					reg = <2>;
					phy-mode = "rev-rmii";
					ethernet = <&fec>;

					fixed-link {
						speed = <100>;
						full-duplex;
					};
				};

				port@3 {
					reg = <3>;
					label = "netright";
					phy-handle = <&switchphy3>;
				};

				port@4 {
					reg = <4>;
					label = "netleft";
					phy-handle = <&switchphy4>;
				};
			};

			mdio {
				#address-cells = <1>;
				#size-cells = <0>;

				switchphy0: switchphy@0 {
					reg = <0>;
					interrupt-parent = <&switch>;
					interrupts = <0 IRQ_TYPE_LEVEL_HIGH>;
				};

				switchphy1: switchphy@1 {
					reg = <1>;
					interrupt-parent = <&switch>;
					interrupts = <1 IRQ_TYPE_LEVEL_HIGH>;
				};

				switchphy2: switchphy@2 {
					reg = <2>;
					interrupt-parent = <&switch>;
					interrupts = <2 IRQ_TYPE_LEVEL_HIGH>;
				};

				switchphy3: switchphy@3 {
					reg = <3>;
					interrupt-parent = <&switch>;
					interrupts = <3 IRQ_TYPE_LEVEL_HIGH>;
				};

				switchphy4: switchphy@4 {
					reg = <4>;
					interrupt-parent = <&switch>;
					interrupts = <4 IRQ_TYPE_LEVEL_HIGH>;
				};
			};
		};
	};
};

&usbh1 {
	vbus-supply = <&reg_5p0v_main>;
	disable-over-current;
	maximum-speed = "full-speed";
	status = "okay";
};

&usbotg {
	vbus-supply = <&reg_5p0v_user_usb>;
	disable-over-current;
	dr_mode = "host";
	status = "okay";
};

&snvs_rtc {
	status = "disabled";
};

&ssi1 {
	status = "okay";
};

&ssi2 {
	status = "okay";
};

&audmux {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_audmux>;
	status = "okay";

	mux-ssi1 {
		fsl,audmux-port = <0>;
		fsl,port-config = <
			(IMX_AUDMUX_V2_PTCR_SYN |
			 IMX_AUDMUX_V2_PTCR_TFSEL(2) |
			 IMX_AUDMUX_V2_PTCR_TCSEL(2) |
			 IMX_AUDMUX_V2_PTCR_TFSDIR |
			 IMX_AUDMUX_V2_PTCR_TCLKDIR)
			IMX_AUDMUX_V2_PDCR_RXDSEL(2)
		>;
	};

	mux-aud3 {
		fsl,audmux-port = <2>;
		fsl,port-config = <
			IMX_AUDMUX_V2_PTCR_SYN
			IMX_AUDMUX_V2_PDCR_RXDSEL(0)
		>;
	};

	mux-ssi2 {
		fsl,audmux-port = <1>;
		fsl,port-config = <
			(IMX_AUDMUX_V2_PTCR_SYN |
			 IMX_AUDMUX_V2_PTCR_TFSEL(4) |
			 IMX_AUDMUX_V2_PTCR_TCSEL(4) |
			 IMX_AUDMUX_V2_PTCR_TFSDIR |
			 IMX_AUDMUX_V2_PTCR_TCLKDIR)
			IMX_AUDMUX_V2_PDCR_RXDSEL(4)
		>;
	};

	mux-aud5 {
		fsl,audmux-port = <4>;
		fsl,port-config = <
			IMX_AUDMUX_V2_PTCR_SYN
			IMX_AUDMUX_V2_PDCR_RXDSEL(1)
		>;
	};
};

&iomuxc {
	pinctrl_accel: accelgrp {
		fsl,pins = <
			MX6QDL_PAD_SD1_CLK__GPIO1_IO20		0x4001b000
		>;
	};

	pinctrl_audmux: audmuxgrp {
		fsl,pins = <
			MX6QDL_PAD_KEY_COL0__AUD5_TXC		0x130b0
			MX6QDL_PAD_KEY_ROW0__AUD5_TXD		0x130b0
			MX6QDL_PAD_KEY_COL1__AUD5_TXFS		0x130b0
			MX6QDL_PAD_CSI0_DAT4__AUD3_TXC		0x130b0
			MX6QDL_PAD_CSI0_DAT5__AUD3_TXD		0x130b0
			MX6QDL_PAD_CSI0_DAT6__AUD3_TXFS		0x130b0
		>;
	};

	pinctrl_codec1: dac1grp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_0__GPIO1_IO00		0x40000038
		>;
	};

	pinctrl_codec2: dac2grp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_2__GPIO1_IO02		0x40000038
		>;
	};

	pinctrl_disp0: disp0grp {
		fsl,pins = <
			MX6QDL_PAD_DI0_DISP_CLK__IPU1_DI0_DISP_CLK 0x100f9
			MX6QDL_PAD_DI0_PIN15__IPU1_DI0_PIN15       0x100f9
			MX6QDL_PAD_DI0_PIN2__IPU1_DI0_PIN02        0x100f9
			MX6QDL_PAD_DI0_PIN3__IPU1_DI0_PIN03        0x100f9
			MX6QDL_PAD_DISP0_DAT0__IPU1_DISP0_DATA00   0x100f9
			MX6QDL_PAD_DISP0_DAT1__IPU1_DISP0_DATA01   0x100f9
			MX6QDL_PAD_DISP0_DAT2__IPU1_DISP0_DATA02   0x100f9
			MX6QDL_PAD_DISP0_DAT3__IPU1_DISP0_DATA03   0x100f9
			MX6QDL_PAD_DISP0_DAT4__IPU1_DISP0_DATA04   0x100f9
			MX6QDL_PAD_DISP0_DAT5__IPU1_DISP0_DATA05   0x100f9
			MX6QDL_PAD_DISP0_DAT6__IPU1_DISP0_DATA06   0x100f9
			MX6QDL_PAD_DISP0_DAT7__IPU1_DISP0_DATA07   0x100f9
			MX6QDL_PAD_DISP0_DAT8__IPU1_DISP0_DATA08   0x100f9
			MX6QDL_PAD_DISP0_DAT9__IPU1_DISP0_DATA09   0x100f9
			MX6QDL_PAD_DISP0_DAT10__IPU1_DISP0_DATA10  0x100f9
			MX6QDL_PAD_DISP0_DAT11__IPU1_DISP0_DATA11  0x100f9
			MX6QDL_PAD_DISP0_DAT12__IPU1_DISP0_DATA12  0x100f9
			MX6QDL_PAD_DISP0_DAT13__IPU1_DISP0_DATA13  0x100f9
			MX6QDL_PAD_DISP0_DAT14__IPU1_DISP0_DATA14  0x100f9
			MX6QDL_PAD_DISP0_DAT15__IPU1_DISP0_DATA15  0x100f9
			MX6QDL_PAD_DISP0_DAT16__IPU1_DISP0_DATA16  0x100f9
			MX6QDL_PAD_DISP0_DAT17__IPU1_DISP0_DATA17  0x100f9
			MX6QDL_PAD_DISP0_DAT18__IPU1_DISP0_DATA18  0x100f9
			MX6QDL_PAD_DISP0_DAT19__IPU1_DISP0_DATA19  0x100f9
			MX6QDL_PAD_DISP0_DAT20__IPU1_DISP0_DATA20  0x100f9
			MX6QDL_PAD_DISP0_DAT21__IPU1_DISP0_DATA21  0x100f9
			MX6QDL_PAD_DISP0_DAT22__IPU1_DISP0_DATA22  0x100f9
			MX6QDL_PAD_DISP0_DAT23__IPU1_DISP0_DATA23  0x100f9
		>;
	};

	pinctrl_ecspi1: ecspi1grp {
		fsl,pins = <
			MX6QDL_PAD_EIM_D17__ECSPI1_MISO		0x100b1
			MX6QDL_PAD_EIM_D18__ECSPI1_MOSI		0x100b1
			MX6QDL_PAD_EIM_D16__ECSPI1_SCLK		0x100b1
			MX6QDL_PAD_EIM_EB2__GPIO2_IO30		0x1b0b1
		>;
	};

	pinctrl_enet: enetgrp {
		fsl,pins = <
			MX6QDL_PAD_ENET_MDC__ENET_MDC		0x000b1
			MX6QDL_PAD_ENET_MDIO__ENET_MDIO		0x100b1
			MX6QDL_PAD_ENET_CRS_DV__ENET_RX_EN	0x100f5
			MX6QDL_PAD_ENET_TX_EN__ENET_TX_EN	0x100f5
			MX6QDL_PAD_ENET_RXD0__ENET_RX_DATA0	0x100c0
			MX6QDL_PAD_ENET_RXD1__ENET_RX_DATA1	0x100c0
			MX6QDL_PAD_ENET_TXD0__ENET_TX_DATA0	0x100f5
			MX6QDL_PAD_ENET_TXD1__ENET_TX_DATA1	0x100f5
			MX6QDL_PAD_GPIO_16__ENET_REF_CLK	0x40010040
			MX6QDL_PAD_ENET_RX_ER__ENET_RX_ER	0x100b0
			MX6QDL_PAD_ENET_REF_CLK__GPIO1_IO23	0x1b0b0
		>;
	};

	pinctrl_gpio3_hog: gpio3hoggrp {
		fsl,pins = <
			MX6QDL_PAD_EIM_D19__GPIO3_IO19		0x1b0b0
			MX6QDL_PAD_EIM_D20__GPIO3_IO20		0x1b0b0
			MX6QDL_PAD_EIM_D22__GPIO3_IO22		0x1b0b0
			MX6QDL_PAD_EIM_D23__GPIO3_IO23		0x1b0b0
		>;
	};

	pinctrl_i2c1: i2c1grp {
		fsl,pins = <
			MX6QDL_PAD_CSI0_DAT8__I2C1_SDA		0x4001b811
			MX6QDL_PAD_CSI0_DAT9__I2C1_SCL		0x4001b811
		>;
	};

	pinctrl_i2c2: i2c2grp {
		fsl,pins = <
			MX6QDL_PAD_KEY_COL3__I2C2_SCL		0x4001b811
			MX6QDL_PAD_KEY_ROW3__I2C2_SDA		0x4001b811
		>;
	};

	pinctrl_i2c3: i2c3grp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_3__I2C3_SCL		0x4001b811
			MX6QDL_PAD_GPIO_6__I2C3_SDA		0x4001b811
		>;
	};

	pinctrl_mdio1: bitbangmdiogrp {
		fsl,pins = <
			/* Bitbang MDIO for DEB Switch */
			MX6QDL_PAD_CSI0_DAT19__GPIO6_IO05	0x4001b030
			MX6QDL_PAD_CSI0_DAT18__GPIO6_IO04	0x40018830
		>;
	};

	pinctrl_pcie: pciegrp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_17__GPIO7_IO12		0x10038
		>;
	};

	pinctrl_pfuze100_irq: pfuze100grp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_18__GPIO7_IO13		0x40010000
		>;
	};

	pinctrl_reg_3p3v_sd: mmcsupply1grp {
		fsl,pins = <
			MX6QDL_PAD_SD3_RST__GPIO7_IO08		0x858
		>;
	};

	pinctrl_rmii_phy_irq: phygrp {
		fsl,pins = <
			MX6QDL_PAD_EIM_D30__GPIO3_IO30		0x40010000
		>;
	};

	pinctrl_switch_irq: switchgrp {
		fsl,pins = <
			MX6QDL_PAD_CSI0_DAT17__GPIO6_IO03	0x4001b000
		>;
	};

	pinctrl_tc358767: tc358767grp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_9__GPIO1_IO09		0x10
		>;
	};

	pinctrl_tpa1: tpa6130-1grp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_4__GPIO1_IO04		0x40000038
		>;
	};

	pinctrl_tpa2: tpa6130-2grp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_5__GPIO1_IO05		0x40000038
		>;
	};

	pinctrl_ts: tsgrp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_8__GPIO1_IO08		0x1b0b0
			MX6QDL_PAD_GPIO_7__GPIO1_IO07		0x1b0b0
		>;
	};

	pinctrl_uart1: uart1grp {
		fsl,pins = <
			MX6QDL_PAD_CSI0_DAT10__UART1_TX_DATA	0x1b0b1
			MX6QDL_PAD_CSI0_DAT11__UART1_RX_DATA	0x1b0b1
		>;
	};

	pinctrl_uart3: uart3grp {
		fsl,pins = <
			MX6QDL_PAD_EIM_D24__UART3_TX_DATA	0x1b0b1
			MX6QDL_PAD_EIM_D25__UART3_RX_DATA	0x1b0b1
			MX6QDL_PAD_EIM_D31__UART3_RTS_B		0x1b0b1
		>;
	};

	pinctrl_uart4: uart4grp {
		fsl,pins = <
			MX6QDL_PAD_CSI0_DAT12__UART4_TX_DATA	0x1b0b1
			MX6QDL_PAD_CSI0_DAT13__UART4_RX_DATA	0x1b0b1
		>;
	};

	pinctrl_ucs1002_pins: ucs1002grp {
		fsl,pins = <
			MX6QDL_PAD_EIM_A25__GPIO5_IO02  	0x1b0b0
			MX6QDL_PAD_EIM_D21__GPIO3_IO21  	0x1b0b0
		>;
	};

	pinctrl_usdhc2: usdhc2grp {
		fsl,pins = <
			MX6QDL_PAD_SD2_CMD__SD2_CMD		0x10059
			MX6QDL_PAD_SD2_CLK__SD2_CLK		0x10069
			MX6QDL_PAD_SD2_DAT0__SD2_DATA0		0x17059
			MX6QDL_PAD_SD2_DAT1__SD2_DATA1		0x17059
			MX6QDL_PAD_SD2_DAT2__SD2_DATA2		0x17059
			MX6QDL_PAD_SD2_DAT3__SD2_DATA3		0x17059
			MX6QDL_PAD_NANDF_D2__GPIO2_IO02		0x40010040
		>;
	};

	pinctrl_usdhc3: usdhc3grp {
		fsl,pins = <
			MX6QDL_PAD_SD3_CMD__SD3_CMD		0x10059
			MX6QDL_PAD_SD3_CLK__SD3_CLK		0x10069
			MX6QDL_PAD_SD3_DAT0__SD3_DATA0		0x17059
			MX6QDL_PAD_SD3_DAT1__SD3_DATA1		0x17059
			MX6QDL_PAD_SD3_DAT2__SD3_DATA2		0x17059
			MX6QDL_PAD_SD3_DAT3__SD3_DATA3		0x17059
			MX6QDL_PAD_NANDF_D0__GPIO2_IO00		0x40010040

		>;
	};

	pinctrl_usdhc4: usdhc4grp {
		fsl,pins = <
			MX6QDL_PAD_SD4_CMD__SD4_CMD		0x17059
			MX6QDL_PAD_SD4_CLK__SD4_CLK		0x10059
			MX6QDL_PAD_SD4_DAT0__SD4_DATA0		0x17059
			MX6QDL_PAD_SD4_DAT1__SD4_DATA1		0x17059
			MX6QDL_PAD_SD4_DAT2__SD4_DATA2		0x17059
			MX6QDL_PAD_SD4_DAT3__SD4_DATA3		0x17059
			MX6QDL_PAD_SD4_DAT4__SD4_DATA4		0x17059
			MX6QDL_PAD_SD4_DAT5__SD4_DATA5		0x17059
			MX6QDL_PAD_SD4_DAT6__SD4_DATA6		0x17059
			MX6QDL_PAD_SD4_DAT7__SD4_DATA7		0x17059
			MX6QDL_PAD_NANDF_ALE__SD4_RESET		0x1b0b1
		>;
	};
};
