// SPDX-License-Identifier: (GPL-2.0 OR MIT)
/*
 * Device tree file for ZII's RPU2 board
 *
 * RPU - Remote Peripheral Unit
 *
 * Copyright (C) 2019 Zodiac Inflight Innovations
 */

/dts-v1/;
#include <dt-bindings/thermal/thermal.h>
#include "imx7d.dtsi"

/ {
	model = "ZII RPU2 Board";
	compatible = "zii,imx7d-rpu2", "fsl,imx7d";

	chosen {
		stdout-path = &uart2;
	};

	cs2000_ref: oscillator {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <24576000>;
	};

	cs2000_in_dummy: dummy-oscillator {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <0>;
	};

	gpio-leds {
		compatible = "gpio-leds";
		pinctrl-0 = <&pinctrl_leds_debug>;
		pinctrl-names = "default";

		led-debug {
			label = "zii:green:debug1";
			gpios = <&gpio2 8 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "heartbeat";
		};
	};

	iio-hwmon {
		compatible = "iio-hwmon";
		io-channels = <&adc1 0>, <&adc1 1>, <&adc1 2>, <&adc1 3>,
			      <&adc2 1>;
	};

	reg_can1_stby: regulator-can1-stby {
		compatible = "regulator-fixed";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_flexcan1_stby>;
		regulator-name = "can1-3v3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		gpio = <&gpio1 9 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};

	reg_can2_stby: regulator-can2-stby {
		compatible = "regulator-fixed";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_flexcan2_stby>;
		regulator-name = "can2-3v3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		gpio = <&gpio1 8 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};

	reg_vref_1v8: regulator-vref-1v8 {
		compatible = "regulator-fixed";
		regulator-name = "vref-1v8";
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
		regulator-always-on;
	};

	reg_3p3v: regulator-3p3v {
		compatible = "regulator-fixed";
		regulator-name = "GEN_3V3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
	};

	reg_5p0v_main: regulator-5p0v-main {
		compatible = "regulator-fixed";
		regulator-name = "5V_MAIN";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		regulator-always-on;
	};

	sound1 {
		compatible = "simple-audio-card";
		simple-audio-card,name = "Audio Output 1";
		simple-audio-card,format = "i2s";
		simple-audio-card,bitclock-master = <&sound1_codec>;
		simple-audio-card,frame-master = <&sound1_codec>;
		simple-audio-card,widgets =
			"Headphone", "Headphone Jack";
		simple-audio-card,routing =
			"Headphone Jack", "HPLEFT",
			"Headphone Jack", "HPRIGHT",
			"LEFTIN", "HPL",
			"RIGHTIN", "HPR";
		simple-audio-card,aux-devs = <&hpa1>;

		simple-audio-card,cpu {
			sound-dai = <&sai1>;
		};

		sound1_codec: simple-audio-card,codec {
			sound-dai = <&codec1>;
			clocks = <&cs2000>;
		};
	};

	sound2 {
		compatible = "simple-audio-card";
		simple-audio-card,name = "Audio Output 2";
		simple-audio-card,format = "i2s";
		simple-audio-card,bitclock-master = <&sound2_codec>;
		simple-audio-card,frame-master = <&sound2_codec>;
		simple-audio-card,widgets =
			"Headphone", "Headphone Jack";
		simple-audio-card,routing =
			"Headphone Jack", "HPLEFT",
			"Headphone Jack", "HPRIGHT",
			"LEFTIN", "HPL",
			"RIGHTIN", "HPR";
		simple-audio-card,aux-devs = <&hpa2>;

		simple-audio-card,cpu {
			sound-dai = <&sai2>;
		};

		sound2_codec: simple-audio-card,codec {
			sound-dai = <&codec2>;
			clocks = <&cs2000>;
		};
	};

	sound3 {
		compatible = "simple-audio-card";
		simple-audio-card,name = "Audio Output 3";
		simple-audio-card,format = "i2s";
		simple-audio-card,bitclock-master = <&sound3_codec>;
		simple-audio-card,frame-master = <&sound3_codec>;
		simple-audio-card,widgets =
			"Headphone", "Headphone Jack";
		simple-audio-card,routing =
			"Headphone Jack", "HPLEFT",
			"Headphone Jack", "HPRIGHT",
			"LEFTIN", "HPL",
			"RIGHTIN", "HPR";
		simple-audio-card,aux-devs = <&hpa3>;

		simple-audio-card,cpu {
			sound-dai = <&sai3>;
		};

		sound3_codec: simple-audio-card,codec {
			sound-dai = <&codec3>;
			clocks = <&cs2000>;
		};
	};
};

&adc1 {
	vref-supply = <&reg_vref_1v8>;
	status = "okay";
};

&adc2 {
	vref-supply = <&reg_vref_1v8>;
	status = "okay";
};

&cpu0 {
	cpu-supply = <&sw1a_reg>;
};

&clks {
	assigned-clocks = <&clks IMX7D_PLL_AUDIO_POST_DIV>;
	assigned-clock-rates = <884736000>;
};

&ecspi1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_ecspi1>;
	cs-gpios = <&gpio4 19 GPIO_ACTIVE_LOW>;
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		spi-max-frequency = <20000000>;
		reg = <0>;
		#address-cells = <1>;
		#size-cells = <1>;
	};
};

&fec1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_enet1>;
	assigned-clocks = <&clks IMX7D_ENET1_TIME_ROOT_SRC>,
			  <&clks IMX7D_ENET1_TIME_ROOT_CLK>;
	assigned-clock-parents = <&clks IMX7D_PLL_ENET_MAIN_100M_CLK>;
	assigned-clock-rates = <0>, <100000000>;
	phy-mode = "rgmii";
	status = "okay";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};

	mdio1: mdio {
		#address-cells = <1>;
		#size-cells = <0>;
		status = "okay";

		switch: switch@0 {
			compatible = "marvell,mv88e6085";
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_switch>;
			reg = <0>;
			eeprom-length = <512>;
			interrupt-parent = <&gpio1>;
			interrupts = <2 IRQ_TYPE_LEVEL_LOW>;
			interrupt-controller;
			#interrupt-cells = <2>;

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;
					label = "eth_cu_1000_1";
				};

				port@1 {
					reg = <1>;
					label = "eth_cu_1000_2";
				};

				port@2 {
					reg = <2>;
					label = "pic";

					fixed-link {
						speed = <100>;
						full-duplex;
					};
				};

				port@5 {
					reg = <5>;
					label = "cpu";
					ethernet = <&fec1>;
					phy-mode = "rgmii-id";

					fixed-link {
						speed = <1000>;
						full-duplex;
					};
				};

				port@6 {
					reg = <6>;
					label = "gigabit_proc";
					ethernet = <&fec2>;
					phy-mode = "rgmii-id";

					fixed-link {
						speed = <1000>;
						full-duplex;
					};
				};
			};
		};
	};
};

&fec2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_enet2>;
	assigned-clocks = <&clks IMX7D_ENET2_TIME_ROOT_SRC>,
			  <&clks IMX7D_ENET2_TIME_ROOT_CLK>;
	assigned-clock-parents = <&clks IMX7D_PLL_ENET_MAIN_100M_CLK>;
	assigned-clock-rates = <0>, <100000000>;
	phy-mode = "rgmii";
	fsl,magic-packet;
	status = "okay";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&flexcan1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_flexcan1>;
	xceiver-supply = <&reg_can1_stby>;
	status = "okay";
};

&flexcan2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_flexcan2>;
	xceiver-supply = <&reg_can2_stby>;
	status = "okay";
};

&gpio1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_gpio1>;

	gpio-line-names = "", "", "", "", "", "", "", "",
			  "", "",
			  "usb_1_en_b",
			  "usb_2_en_b",
			  "", "", "", "", "", "", "", "",
			  "", "", "", "", "", "", "", "",
			  "", "", "", "";
};

&gpio2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_gpio2>;

	gpio-line-names = "12v_out_en_1",
			  "12v_out_en_2",
			  "12v_out_en_3",
			  "28v_out_en_5",
			  "28v_out_en_1",
			  "28v_out_en_2",
			  "28v_out_en_3",
			  "28v_out_en_4",
			  "", "",
			  "usb_3_en_b",
			  "usb_4_en_b",
			  "", "", "", "", "", "", "", "",
			  "", "", "", "", "", "", "", "",
			  "", "", "", "";
};

&i2c1 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c1>;
	status = "okay";

	pmic: pmic@8 {
		compatible = "fsl,pfuze3000";
		reg = <0x08>;

		regulators {
			sw1a_reg: sw1a {
				regulator-min-microvolt = <700000>;
				regulator-max-microvolt = <3300000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-ramp-delay = <6250>;
			};

			sw1c_reg: sw1b {
				regulator-min-microvolt = <700000>;
				regulator-max-microvolt = <1475000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-ramp-delay = <6250>;
			};

			sw2_reg: sw2 {
				regulator-min-microvolt = <1500000>;
				regulator-max-microvolt = <1850000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw3a_reg: sw3 {
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <1650000>;
				regulator-boot-on;
				regulator-always-on;
			};

			swbst_reg: swbst {
				regulator-min-microvolt = <5000000>;
				regulator-max-microvolt = <5150000>;
			};

			snvs_reg: vsnvs {
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <3000000>;
				regulator-boot-on;
				regulator-always-on;
			};

			vref_reg: vrefddr {
				regulator-boot-on;
				regulator-always-on;
			};

			vgen1_reg: vldo1 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen2_reg: vldo2 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1550000>;
				regulator-always-on;
			};

			vgen3_reg: vccsd {
				regulator-min-microvolt = <2850000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen4_reg: v33 {
				regulator-min-microvolt = <2850000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen5_reg: vldo3 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen6_reg: vldo4 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};
		};
	};

	cs2000: clkgen@4e {
		compatible = "cirrus,cs2000-cp";
		reg = <0x4e>;
		#clock-cells = <0>;
		clock-names = "clk_in", "ref_clk";
		clocks = <&cs2000_in_dummy>, <&cs2000_ref>;
		assigned-clocks = <&cs2000>;
		assigned-clock-rates = <24000000>;
	};

	eeprom@50 {
		compatible = "atmel,24c04";
		reg = <0x50>;
	};

	eeprom@52 {
		compatible = "atmel,24c04";
		reg = <0x52>;
	};
};

&i2c2 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c2>;
	status = "okay";

	codec2: codec@18 {
		compatible = "ti,tlv320dac3100";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_codec2>;
		reg = <0x18>;
		#sound-dai-cells = <0>;
		HPVDD-supply = <&reg_3p3v>;
		SPRVDD-supply = <&reg_3p3v>;
		SPLVDD-supply = <&reg_3p3v>;
		AVDD-supply = <&reg_3p3v>;
		IOVDD-supply = <&reg_3p3v>;
		DVDD-supply = <&vgen4_reg>;
		gpio-reset = <&gpio1 6 GPIO_ACTIVE_LOW>;
	};

	hpa2: amp@60 {
		compatible = "ti,tpa6130a2";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_tpa2>;
		reg = <0x60>;
		power-gpio = <&gpio3 27 GPIO_ACTIVE_HIGH>;
		Vdd-supply = <&reg_5p0v_main>;
	};
};

&i2c3 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c3>;
	status = "okay";

	codec3: codec@18 {
		compatible = "ti,tlv320dac3100";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_codec3>;
		reg = <0x18>;
		#sound-dai-cells = <0>;
		HPVDD-supply = <&reg_3p3v>;
		SPRVDD-supply = <&reg_3p3v>;
		SPLVDD-supply = <&reg_3p3v>;
		AVDD-supply = <&reg_3p3v>;
		IOVDD-supply = <&reg_3p3v>;
		DVDD-supply = <&vgen4_reg>;
		gpio-reset = <&gpio1 7 GPIO_ACTIVE_LOW>;
	};

	hpa3: amp@60 {
		compatible = "ti,tpa6130a2";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_tpa3>;
		reg = <0x60>;
		power-gpio = <&gpio3 28 GPIO_ACTIVE_HIGH>;
		Vdd-supply = <&reg_5p0v_main>;
	};
};

&i2c4 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c4>;
	status = "okay";

	codec1: codec@18 {
		compatible = "ti,tlv320dac3100";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_codec1>;
		reg = <0x18>;
		#sound-dai-cells = <0>;
		HPVDD-supply = <&reg_3p3v>;
		SPRVDD-supply = <&reg_3p3v>;
		SPLVDD-supply = <&reg_3p3v>;
		AVDD-supply = <&reg_3p3v>;
		IOVDD-supply = <&reg_3p3v>;
		DVDD-supply = <&vgen4_reg>;
		gpio-reset = <&gpio1 5 GPIO_ACTIVE_LOW>;
	};

	hpa1: amp@60 {
		compatible = "ti,tpa6130a2";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_tpa1>;
		reg = <0x60>;
		power-gpio = <&gpio3 26 GPIO_ACTIVE_HIGH>;
		Vdd-supply = <&reg_5p0v_main>;
	};
};

&sai1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_sai1>;
	assigned-clocks = <&clks IMX7D_SAI1_ROOT_SRC>,
			  <&clks IMX7D_SAI1_ROOT_CLK>;
	assigned-clock-parents = <&clks IMX7D_PLL_AUDIO_POST_DIV>;
	assigned-clock-rates = <0>, <36864000>;
	status = "okay";
};

&sai2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_sai2>;
	assigned-clocks = <&clks IMX7D_SAI2_ROOT_SRC>,
			  <&clks IMX7D_SAI2_ROOT_CLK>;
	assigned-clock-parents = <&clks IMX7D_PLL_AUDIO_POST_DIV>;
	assigned-clock-rates = <0>, <36864000>;
	status = "okay";
};

&sai3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_sai3>;
	assigned-clocks = <&clks IMX7D_SAI3_ROOT_SRC>,
			  <&clks IMX7D_SAI3_ROOT_CLK>;
	assigned-clock-parents = <&clks IMX7D_PLL_AUDIO_POST_DIV>;
	assigned-clock-rates = <0>, <36864000>;
	status = "okay";
};

&uart2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart2>;
	assigned-clocks = <&clks IMX7D_UART2_ROOT_SRC>;
	assigned-clock-parents = <&clks IMX7D_OSC_24M_CLK>;
	status = "okay";
};

&uart4 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart4>;
	assigned-clocks = <&clks IMX7D_UART4_ROOT_SRC>;
	assigned-clock-parents = <&clks IMX7D_PLL_SYS_MAIN_240M_CLK>;
	status = "okay";

	mcu {
		compatible = "zii,rave-sp-rdu2";
		current-speed = <1000000>;
		#address-cells = <1>;
		#size-cells = <1>;

		watchdog {
			compatible = "zii,rave-sp-watchdog";
		};

		eeprom@a3 {
			compatible = "zii,rave-sp-eeprom";
			reg = <0xa3 0x4000>;
			#address-cells = <1>;
			#size-cells = <1>;
			zii,eeprom-name = "main-eeprom";
		};
	};
};

&usbotg1 {
	dr_mode = "host";
	disable-over-current;
	status = "okay";
};

&usbotg2 {
	dr_mode = "host";
	disable-over-current;
	status = "okay";
};

&usdhc1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc1>;
	bus-width = <4>;
	no-1-8-v;
	no-sdio;
	keep-power-in-suspend;
	status = "okay";
};

&usdhc3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc3>;
	bus-width = <8>;
	no-1-8-v;
	non-removable;
	no-sdio;
	no-sd;
	keep-power-in-suspend;
	status = "okay";
};

&wdog1 {
	status = "disabled";
};

&snvs_rtc {
	status = "disabled";
};

&iomuxc {
	pinctrl_ecspi1: ecspi1grp {
		fsl,pins = <
			MX7D_PAD_ECSPI1_SCLK__ECSPI1_SCLK	0x2
			MX7D_PAD_ECSPI1_MOSI__ECSPI1_MOSI	0x2
			MX7D_PAD_ECSPI1_MISO__ECSPI1_MISO	0x2
			MX7D_PAD_ECSPI1_SS0__GPIO4_IO19         0x59
		>;
	};

	pinctrl_enet1: enet1grp {
		fsl,pins = <
			MX7D_PAD_SD2_CD_B__ENET1_MDIO				0x3
			MX7D_PAD_SD2_WP__ENET1_MDC				0x3
			MX7D_PAD_ENET1_RGMII_TXC__ENET1_RGMII_TXC		0x1
			MX7D_PAD_ENET1_RGMII_TD0__ENET1_RGMII_TD0		0x1
			MX7D_PAD_ENET1_RGMII_TD1__ENET1_RGMII_TD1		0x1
			MX7D_PAD_ENET1_RGMII_TD2__ENET1_RGMII_TD2		0x1
			MX7D_PAD_ENET1_RGMII_TD3__ENET1_RGMII_TD3		0x1
			MX7D_PAD_ENET1_RGMII_TX_CTL__ENET1_RGMII_TX_CTL		0x1
			MX7D_PAD_ENET1_RGMII_RXC__ENET1_RGMII_RXC		0x1
			MX7D_PAD_ENET1_RGMII_RD0__ENET1_RGMII_RD0		0x1
			MX7D_PAD_ENET1_RGMII_RD1__ENET1_RGMII_RD1		0x1
			MX7D_PAD_ENET1_RGMII_RD2__ENET1_RGMII_RD2		0x1
			MX7D_PAD_ENET1_RGMII_RD3__ENET1_RGMII_RD3		0x1
			MX7D_PAD_ENET1_RGMII_RX_CTL__ENET1_RGMII_RX_CTL		0x1
		>;
	};

	pinctrl_enet2: enet2grp {
		fsl,pins = <
			MX7D_PAD_EPDC_GDSP__ENET2_RGMII_TXC			0x1
			MX7D_PAD_EPDC_SDCE2__ENET2_RGMII_TD0			0x1
			MX7D_PAD_EPDC_SDCE3__ENET2_RGMII_TD1			0x1
			MX7D_PAD_EPDC_GDCLK__ENET2_RGMII_TD2			0x1
			MX7D_PAD_EPDC_GDOE__ENET2_RGMII_TD3			0x1
			MX7D_PAD_EPDC_GDRL__ENET2_RGMII_TX_CTL			0x1
			MX7D_PAD_EPDC_SDCE1__ENET2_RGMII_RXC			0x1
			MX7D_PAD_EPDC_SDCLK__ENET2_RGMII_RD0			0x1
			MX7D_PAD_EPDC_SDLE__ENET2_RGMII_RD1			0x1
			MX7D_PAD_EPDC_SDOE__ENET2_RGMII_RD2			0x1
			MX7D_PAD_EPDC_SDSHR__ENET2_RGMII_RD3			0x1
			MX7D_PAD_EPDC_SDCE0__ENET2_RGMII_RX_CTL			0x1
			MX7D_PAD_UART1_TX_DATA__ENET2_1588_EVENT0_OUT		0x1
		>;
	};

	pinctrl_flexcan1: flexcan1grp {
		fsl,pins = <
			MX7D_PAD_GPIO1_IO12__FLEXCAN1_RX	0x59
			MX7D_PAD_GPIO1_IO13__FLEXCAN1_TX	0x59
		>;
	};

	pinctrl_flexcan1_stby: flexcan1stbygrp {
		fsl,pins = <
			MX7D_PAD_GPIO1_IO08__GPIO1_IO8		0x59
		>;
	};

	pinctrl_flexcan2: flexcan2grp {
		fsl,pins = <
			MX7D_PAD_GPIO1_IO14__FLEXCAN2_RX	0x59
			MX7D_PAD_GPIO1_IO15__FLEXCAN2_TX	0x59
		>;
	};

	pinctrl_flexcan2_stby: flexcan2stbygrp {
		fsl,pins = <
			MX7D_PAD_GPIO1_IO09__GPIO1_IO9		0x59
		>;
	};

	pinctrl_gpio1: gpio1grp {
		fsl,pins = <
			MX7D_PAD_GPIO1_IO10__GPIO1_IO10		0x00
			MX7D_PAD_GPIO1_IO11__GPIO1_IO11		0x00
		>;
	};

	pinctrl_gpio2: gpio2grp {
		fsl,pins = <
			MX7D_PAD_EPDC_DATA00__GPIO2_IO0		0x00
			MX7D_PAD_EPDC_DATA01__GPIO2_IO1		0x00
			MX7D_PAD_EPDC_DATA02__GPIO2_IO2		0x00
			MX7D_PAD_EPDC_DATA03__GPIO2_IO3		0x03
			MX7D_PAD_EPDC_DATA04__GPIO2_IO4		0x03
			MX7D_PAD_EPDC_DATA05__GPIO2_IO5		0x03
			MX7D_PAD_EPDC_DATA06__GPIO2_IO6		0x03
			MX7D_PAD_EPDC_DATA07__GPIO2_IO7		0x03
			MX7D_PAD_EPDC_DATA10__GPIO2_IO10	0x00
			MX7D_PAD_EPDC_DATA11__GPIO2_IO11	0x00
		>;
	};

	pinctrl_i2c1: i2c1grp {
		fsl,pins = <
			MX7D_PAD_I2C1_SDA__I2C1_SDA		0x4000007f
			MX7D_PAD_I2C1_SCL__I2C1_SCL		0x4000007f
		>;
	};

	pinctrl_i2c2: i2c2grp {
		fsl,pins = <
			MX7D_PAD_I2C2_SDA__I2C2_SDA		0x4000007f
			MX7D_PAD_I2C2_SCL__I2C2_SCL		0x4000007f
		>;
	};

	pinctrl_i2c3: i2c3grp {
		fsl,pins = <
			MX7D_PAD_I2C3_SDA__I2C3_SDA		0x4000007f
			MX7D_PAD_I2C3_SCL__I2C3_SCL		0x4000007f
		>;
	};

	pinctrl_i2c3_gpio: i2c3gpiogrp {
		fsl,pins = <
			MX7D_PAD_I2C3_SDA__GPIO4_IO13		0x4000007f
			MX7D_PAD_I2C3_SCL__GPIO4_IO12		0x4000007f
		>;
	};

	pinctrl_i2c4: i2c4grp {
		fsl,pins = <
			MX7D_PAD_I2C4_SDA__I2C4_SDA		0x4000007f
			MX7D_PAD_I2C4_SCL__I2C4_SCL		0x4000007f
		>;
	};

	pinctrl_i2c4_gpio: i2c4gpiogrp {
		fsl,pins = <
			MX7D_PAD_SAI1_RX_BCLK__GPIO6_IO17	0x4000007f
			MX7D_PAD_SAI1_RX_SYNC__GPIO6_IO16	0x4000007f
		>;
	};

	pinctrl_leds_debug: debuggrp {
		fsl,pins = <
			MX7D_PAD_EPDC_DATA08__GPIO2_IO8		0x59
		>;
	};

	pinctrl_sai1: sai1grp {
		fsl,pins = <
			MX7D_PAD_SAI1_TX_BCLK__SAI1_TX_BCLK	0x1f
			MX7D_PAD_SAI1_TX_SYNC__SAI1_TX_SYNC	0x1f
			MX7D_PAD_SAI1_TX_DATA__SAI1_TX_DATA0	0x30
		>;
	};

	pinctrl_sai2: sai2grp {
		fsl,pins = <
			MX7D_PAD_SAI2_TX_BCLK__SAI2_TX_BCLK	0x1f
			MX7D_PAD_SAI2_TX_SYNC__SAI2_TX_SYNC	0x1f
			MX7D_PAD_SAI2_TX_DATA__SAI2_TX_DATA0	0x30
		>;
	};

	pinctrl_sai3: sai3grp {
		fsl,pins = <
			MX7D_PAD_UART3_TX_DATA__SAI3_TX_BCLK	0x1f
			MX7D_PAD_UART3_CTS_B__SAI3_TX_SYNC	0x1f
			MX7D_PAD_UART3_RTS_B__SAI3_TX_DATA0	0x30
		>;
	};

	pinctrl_tpa1: tpa6130-1grp {
		fsl,pins = <
			MX7D_PAD_LCD_DATA21__GPIO3_IO26		0x40000038
		>;
	};

	pinctrl_tpa2: tpa6130-2grp {
		fsl,pins = <
			MX7D_PAD_LCD_DATA22__GPIO3_IO27		0x40000038
		>;
	};

	pinctrl_tpa3: tpa6130-3grp {
		fsl,pins = <
			MX7D_PAD_LCD_DATA23__GPIO3_IO28		0x40000038
		>;
	};

	pinctrl_uart2: uart2grp {
		fsl,pins = <
			MX7D_PAD_UART2_RX_DATA__UART2_DCE_RX	0x79
			MX7D_PAD_UART2_TX_DATA__UART2_DCE_TX	0x79
		>;
	};

	pinctrl_uart4: uart4grp {
		fsl,pins = <
			MX7D_PAD_SD2_DATA0__UART4_DCE_RX	0x79
			MX7D_PAD_SD2_DATA1__UART4_DCE_TX	0x79
		>;
	};

	pinctrl_usdhc1: usdhc1grp {
		fsl,pins = <
			MX7D_PAD_SD1_CMD__SD1_CMD		0x59
			MX7D_PAD_SD1_CLK__SD1_CLK		0x19
			MX7D_PAD_SD1_DATA0__SD1_DATA0		0x59
			MX7D_PAD_SD1_DATA1__SD1_DATA1		0x59
			MX7D_PAD_SD1_DATA2__SD1_DATA2		0x59
			MX7D_PAD_SD1_DATA3__SD1_DATA3		0x59
		>;
	};

	pinctrl_usdhc3: usdhc3grp {
		fsl,pins = <
			MX7D_PAD_SD3_CMD__SD3_CMD		0x59
			MX7D_PAD_SD3_CLK__SD3_CLK		0x19
			MX7D_PAD_SD3_DATA0__SD3_DATA0		0x59
			MX7D_PAD_SD3_DATA1__SD3_DATA1		0x59
			MX7D_PAD_SD3_DATA2__SD3_DATA2		0x59
			MX7D_PAD_SD3_DATA3__SD3_DATA3		0x59
			MX7D_PAD_SD3_DATA4__SD3_DATA4		0x59
			MX7D_PAD_SD3_DATA5__SD3_DATA5		0x59
			MX7D_PAD_SD3_DATA6__SD3_DATA6		0x59
			MX7D_PAD_SD3_DATA7__SD3_DATA7		0x59
			MX7D_PAD_SD3_RESET_B__SD3_RESET_B	0x59
		>;
	};
};

&iomuxc_lpsr {
	pinctrl_codec1: dac1grp {
		fsl,pins = <
			MX7D_PAD_LPSR_GPIO1_IO05__GPIO1_IO5	0x40000038
		>;
	};

	pinctrl_codec2: dac2grp {
		fsl,pins = <
			MX7D_PAD_LPSR_GPIO1_IO06__GPIO1_IO6	0x40000038
		>;
	};

	pinctrl_codec3: dac3grp {
		fsl,pins = <
			MX7D_PAD_LPSR_GPIO1_IO07__GPIO1_IO7	0x40000038
		>;
	};

	pinctrl_switch: switchgrp {
		fsl,pins = <
			MX7D_PAD_LPSR_GPIO1_IO02__GPIO1_IO2	0x08
		>;
	};
};
