* Marvell PXA1928 USB and HSIC PHYs

Required properties:
- compatible: "marvell,pxa1928-usb-phy" or "marvell,pxa1928-hsic-phy"
- reg: base address and length of the registers
- clocks - A single clock. From common clock binding.
- #phys-cells: should be 0. From common phy binding.
- resets: reference to the reset controller

Example:

	usbphy: phy@7000 {
		compatible = "marvell,pxa1928-usb-phy";
		reg = <0x7000 0xe0>;
		clocks = <&apmu_clocks PXA1928_CLK_USB>;
		#phy-cells = <0>;
	};

