Amlogic Meson6/Meson8/Meson8b bootrom:
--------------------------------------

The bootrom register area can be used to access SoC specific
information, such as the "misc version".

Required properties:
- reg: the register range of the bootrom registers
- compatible: should be "amlogic,meson-mx-bootrom" along with "syscon"


Example:

	bootrom: bootrom@d9040000 {
		compatible = "amlogic,meson-mx-bootrom", "syscon";
		reg = <0xd9040000 0x10000>;
	};
