* MAXI MAX11801 Resistive touch screen controller with i2c interface

Required properties:
- compatible: must be "maxim,max11801"
- reg: i2c slave address
- interrupts: touch controller interrupt

Example:

&i2c1 {
	max11801: touchscreen@48 {
		compatible = "maxim,max11801";
		reg = <0x48>;
		interrupt-parent = <&gpio3>;
		interrupts = <31 IRQ_TYPE_EDGE_FALLING>;
	};
};
