Freescale Vybrid Miscellaneous System Control - CPU Configuration

The MSCM IP contains multiple sub modules, this binding describes the first
block of registers which contains CPU configuration information.

Required properties:
- compatible:	"fsl,vf610-mscm-cpucfg", "syscon"
- reg:		the register range of the MSCM CPU configuration registers

Example:
	mscm_cpucfg: cpucfg@40001000 {
		compatible = "fsl,vf610-mscm-cpucfg", "syscon";
		reg = <0x40001000 0x800>;
	}
