RT1015 Mono Class D Audio Amplifier

This device supports I2C only.

Required properties:

- compatible : "realtek,rt1015".

- reg : The I2C address of the device.

Optional properties:

- realtek,power-up-delay-ms
  Set a delay time for flush work to be completed,
  this value is adjustable depending on platform.

Example:

rt1015: codec@28 {
	compatible = "realtek,rt1015";
	reg = <0x28>;
	realtek,power-up-delay-ms = <50>;
};
