* NXP LPC32xx SoC High Speed UART

Required properties:
- compatible: Should be "nxp,lpc3220-hsuart"
- reg: Should contain registers location and length
- interrupts: Should contain interrupt

Example:

	uart1: serial@40014000 {
		compatible = "nxp,lpc3220-hsuart";
		reg = <0x40014000 0x1000>;
		interrupts = <26 0>;
	};
