* NXP LPC18xx OTP memory

Internal OTP (One Time Programmable) memory for NXP LPC18xx/43xx devices.

Required properties:
  - compatible: Should be "nxp,lpc1850-otp"
  - reg: Must contain an entry with the physical base address and length
    for each entry in reg-names.
  - address-cells: must be set to 1.
  - size-cells: must be set to 1.

See nvmem.txt for more information.

Example:
  otp: otp@40045000 {
    compatible = "nxp,lpc1850-otp";
    reg = <0x40045000 0x1000>;
    #address-cells = <1>;
    #size-cells = <1>;
  };
