MediaTek CAMSYS controller
============================

The MediaTek camsys controller provides various clocks to the system.

Required Properties:

- compatible: Should be one of:
	- "mediatek,mt6765-camsys", "syscon"
	- "mediatek,mt6779-camsys", "syscon"
	- "mediatek,mt8183-camsys", "syscon"
- #clock-cells: Must be 1

The camsys controller uses the common clk binding from
Documentation/devicetree/bindings/clock/clock-bindings.txt
The available clocks are defined in dt-bindings/clock/mt*-clk.h.

Example:

camsys: camsys@1a000000  {
	compatible = "mediatek,mt8183-camsys", "syscon";
	reg = <0 0x1a000000  0 0x1000>;
	#clock-cells = <1>;
};
