RT5616 audio CODEC

This device supports I2C only.

Required properties:

- compatible : "realtek,rt5616".

- reg : The I2C address of the device.

Optional properties:

- clocks: The phandle of the master clock to the CODEC.

- clock-names: Should be "mclk".

Pins on the device (for linking into audio routes) for RT5616:

  * IN1P
  * IN2P
  * IN2N
  * LOUTL
  * LOUTR
  * HPOL
  * HPOR

Example:

rt5616: codec@1b {
	compatible = "realtek,rt5616";
	reg = <0x1b>;
};
