EPSON TOYOCOM RTC-7301SF/DG

Required properties:

- compatible: Should be "epson,rtc7301sf" or "epson,rtc7301dg"
- reg: Specifies base physical address and size of the registers.
- interrupts: A single interrupt specifier.

Example:

rtc: rtc@44a00000 {
	compatible = "epson,rtc7301dg";
	reg = <0x44a00000 0x10000>;
	interrupt-parent = <&axi_intc_0>;
	interrupts = <3 2>;
};
