Lantiq GSWIP Ethernet switches
==================================

Required properties for GSWIP core:

- compatible	: "lantiq,xrx200-gswip" for the embedded GSWIP in the
		  xRX200 SoC
		  "lantiq,xrx300-gswip" for the embedded GSWIP in the
		  xRX300 SoC
		  "lantiq,xrx330-gswip" for the embedded GSWIP in the
		  xRX330 SoC
- reg		: memory range of the GSWIP core registers
		: memory range of the GSWIP MDIO registers
		: memory range of the GSWIP MII registers

See Documentation/devicetree/bindings/net/dsa/dsa.txt for a list of
additional required and optional properties.


Required properties for MDIO bus:
- compatible	: "lantiq,xrx200-mdio" for the MDIO bus inside the GSWIP
		  core of the xRX200 SoC and the PHYs connected to it.

See Documentation/devicetree/bindings/net/mdio.txt for a list of additional
required and optional properties.


Required properties for GPHY firmware loading:
- compatible	: "lantiq,xrx200-gphy-fw", "lantiq,gphy-fw"
		  "lantiq,xrx300-gphy-fw", "lantiq,gphy-fw"
		  "lantiq,xrx330-gphy-fw", "lantiq,gphy-fw"
		  for the loading of the firmware into the embedded
		  GPHY core of the SoC.
- lantiq,rcu	: reference to the rcu syscon

The GPHY firmware loader has a list of GPHY entries, one for each
embedded GPHY

- reg		: Offset of the GPHY firmware register in the RCU
		  register range
- resets	: list of resets of the embedded GPHY
- reset-names	: list of names of the resets

Example:

Ethernet switch on the VRX200 SoC:

switch@e108000 {
	#address-cells = <1>;
	#size-cells = <0>;
	compatible = "lantiq,xrx200-gswip";
	reg = <	0xe108000 0x3100	/* switch */
		0xe10b100 0xd8		/* mdio */
		0xe10b1d8 0x130		/* mii */
		>;
	dsa,member = <0 0>;

	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@0 {
			reg = <0>;
			label = "lan3";
			phy-mode = "rgmii";
			phy-handle = <&phy0>;
		};

		port@1 {
			reg = <1>;
			label = "lan4";
			phy-mode = "rgmii";
			phy-handle = <&phy1>;
		};

		port@2 {
			reg = <2>;
			label = "lan2";
			phy-mode = "internal";
			phy-handle = <&phy11>;
		};

		port@4 {
			reg = <4>;
			label = "lan1";
			phy-mode = "internal";
			phy-handle = <&phy13>;
		};

		port@5 {
			reg = <5>;
			label = "wan";
			phy-mode = "rgmii";
			phy-handle = <&phy5>;
		};

		port@6 {
			reg = <0x6>;
			ethernet = <&eth0>;
		};
	};

	mdio {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "lantiq,xrx200-mdio";
		reg = <0>;

		phy0: ethernet-phy@0 {
			reg = <0x0>;
		};
		phy1: ethernet-phy@1 {
			reg = <0x1>;
		};
		phy5: ethernet-phy@5 {
			reg = <0x5>;
		};
		phy11: ethernet-phy@11 {
			reg = <0x11>;
		};
		phy13: ethernet-phy@13 {
			reg = <0x13>;
		};
	};

	gphy-fw {
		compatible = "lantiq,xrx200-gphy-fw", "lantiq,gphy-fw";
		lantiq,rcu = <&rcu0>;
		#address-cells = <1>;
		#size-cells = <0>;

		gphy@20 {
			reg = <0x20>;

			resets = <&reset0 31 30>;
			reset-names = "gphy";
		};

		gphy@68 {
			reg = <0x68>;

			resets = <&reset0 29 28>;
			reset-names = "gphy";
		};
	};
};
