STMicroelectronics STM32 Peripheral Reset Controller
====================================================

The RCC IP is both a reset and a clock controller.

Please see Documentation/devicetree/bindings/clock/st,stm32-rcc.txt
