* Dialog Semiconductor DA9210 Multi-phase 12A DCDC BUCK Converter

Required properties:

- compatible:	must be "dlg,da9210"
- reg:		the i2c slave address of the regulator. It should be 0x68.

Optional properties:

- interrupts:	a reference to the DA9210 interrupt, if available.

Any standard regulator properties can be used to configure the single da9210
DCDC.

Example:

	da9210@68 {
		compatible = "dlg,da9210";
		reg = <0x68>;

		interrupt-parent = <...>;
		interrupts = <...>;

		regulator-min-microvolt = <300000>;
		regulator-max-microvolt = <1570000>;
		regulator-min-microamp = <1600000>;
		regulator-max-microamp = <4600000>;
		regulator-boot-on;
	};
