Actions Semi Owl UART

Required properties:
- compatible :  "actions,s500-uart", "actions,owl-uart" for S500
                "actions,s900-uart", "actions,owl-uart" for S900
- reg        :  Offset and length of the register set for the device.
- interrupts :  Should contain UART interrupt.


Example:

		uart3: serial@b0126000 {
			compatible = "actions,s500-uart", "actions,owl-uart";
			reg = <0xb0126000 0x1000>;
			interrupts = <GIC_SPI 32 IRQ_TYPE_LEVEL_HIGH>;
		};
