Motorola CPCAP PMIC voltage regulators
------------------------------------

Requires node properties:
- "compatible" value one of:
    "motorola,cpcap-regulator"
    "motorola,mapphone-cpcap-regulator"
    "motorola,xoom-cpcap-regulator"

Required regulator properties:
- "regulator-name"
- "regulator-enable-ramp-delay"
- "regulator-min-microvolt"
- "regulator-max-microvolt"

Optional regulator properties:
- "regulator-boot-on"

See Documentation/devicetree/bindings/regulator/regulator.txt
for more details about the regulator properties.

Example:

cpcap_regulator: regulator {
	compatible = "motorola,cpcap-regulator";

	cpcap_regulators: regulators {
		sw5: SW5 {
			regulator-min-microvolt = <5050000>;
			regulator-max-microvolt = <5050000>;
			regulator-enable-ramp-delay = <50000>;
			regulator-boot-on;
		};
	};
};
