* Dialog DA9062/61 TJUNC Thermal Module

This module is part of the DA9061/DA9062. For more details about entire
DA9062 and DA9061 chips see Documentation/devicetree/bindings/mfd/da9062.txt

Junction temperature thermal module uses an interrupt signal to identify
high THERMAL_TRIP_HOT temperatures for the PMIC device.

Required properties:

- compatible: should be one of the following valid compatible string lines:
        "dlg,da9061-thermal", "dlg,da9062-thermal"
        "dlg,da9062-thermal"

Optional properties:

- polling-delay-passive : Specify the polling period, measured in
    milliseconds, between thermal zone device update checks.

Example: DA9062

	pmic0: da9062@58 {
		thermal {
			compatible = "dlg,da9062-thermal";
			polling-delay-passive = <3000>;
		};
	};

Example: DA9061 using a fall-back compatible for the DA9062 onkey driver

	pmic0: da9061@58 {
		thermal {
			compatible = "dlg,da9061-thermal", "dlg,da9062-thermal";
			polling-delay-passive = <3000>;
		};
	};
