Krait Clock Controller

PROPERTIES

- compatible:
	Usage: required
	Value type: <string>
	Definition: must be one of:
			"qcom,krait-cc-v1"
			"qcom,krait-cc-v2"

- #clock-cells:
	Usage: required
	Value type: <u32>
	Definition: must be 1

- clocks:
	Usage: required
	Value type: <prop-encoded-array>
	Definition: reference to the clock parents of hfpll, secondary muxes.

- clock-names:
	Usage: required
	Value type: <stringlist>
	Definition: must be "hfpll0", "hfpll1", "acpu0_aux", "acpu1_aux", "qsb".

Example:

	kraitcc: clock-controller {
		compatible = "qcom,krait-cc-v1";
		clocks = <&hfpll0>, <&hfpll1>, <&acpu0_aux>, <&acpu1_aux>, <qsb>;
		clock-names = "hfpll0", "hfpll1", "acpu0_aux", "acpu1_aux", "qsb";
		#clock-cells = <1>;
	};
