* VIA Rhine 10/100 Network Controller

Required properties:
- compatible : Should be "via,vt8500-rhine" for integrated
	Rhine controllers found in VIA VT8500, WonderMedia WM8950
	and similar. These are listed as 1106:3106 rev. 0x84 on the
	virtual PCI bus under vendor-provided kernels
- reg : Address and length of the io space
- interrupts : Should contain the controller interrupt line

Examples:

ethernet@d8004000 {
	compatible = "via,vt8500-rhine";
	reg = <0xd8004000 0x100>;
	interrupts = <10>;
};
