What:		/sys/bus/fsi/devices/XX.XX.00:06/sbefifoX/timeout
KernelVersion:	5.15
Contact:	eajames@linux.ibm.com
Description:
		Indicates whether or not this SBE device has experienced a
		timeout; i.e. the SBE did not respond within the time allotted
		by the driver. A value of 1 indicates that a timeout has
		occurred and no transfers have completed since the timeout. A
		value of 0 indicates that no timeout has occurred, or if one
		has, more recent transfers have completed successfully.
