Realtek RTD129x Real-Time Clock
===============================

Required properties:
- compatible :  Should be "realtek,rtd1295-rtc"
- reg        :  Specifies the physical base address and size
- clocks     :  Specifies the clock gate


Example:

	rtc@9801b600 {
		compatible = "realtek,rtd1295-clk";
		reg = <0x9801b600 0x100>;
		clocks = <&clkc RTD1295_CLK_EN_MISC_RTC>;
	};
