Cadence Xtensa XTFPGA platform SPI controller.

This simple SPI master controller is built into xtfpga bitstreams and is used
to control daughterboard audio codec.

Required properties:
- compatible: should be "cdns,xtfpga-spi".
- reg: physical base address of the controller and length of memory mapped
  region.
