What:		/sys/.../iio:deviceX/in_capacitableY_calibbias_calibration
What:		/sys/.../iio:deviceX/in_capacitableY_calibscale_calibration
KernelVersion:	6.1
Contact:	linux-iio@vger.kernel.org
Description:
		Write 1 to trigger a calibration of the calibbias or
		calibscale. For calibscale, a full scale capacitance should
		be connected to the capacitance input and a
		calibscale_calibration then started.  For calibbias see
		the device datasheet section on "capacitive system offset
		calibration".
