What:		/sys/bus/iio/devices/iio:deviceX/out_current_heater_raw
What:		/sys/bus/iio/devices/iio:deviceX/out_current_heater_raw_available
KernelVersion:	5.3.8
Contact:	linux-iio@vger.kernel.org
Description:
		Controls the heater device within the humidity sensor to get
		rid of excess condensation.

		In some devices, this is just a switch in which case 0 = OFF,
		and 1 = ON.
