What: /sys/bus/platform/devices/*twl4030-usb/vbus
Description:
	Read-only status reporting if VBUS (approx 5V)
	is being supplied by the USB bus.

	Possible values: "on", "off".

	Changes are notified via select/poll.
