.. SPDX-License-Identifier: GFDL-1.1-no-invariants-or-later

.. _V4L2-TCH-FMT-TU08:

**************************
V4L2_TCH_FMT_TU08 ('TU08')
**************************

*man V4L2_TCH_FMT_TU08(2)*

8-bit unsigned raw touch data

Description
===========

This format represents unsigned 8-bit data from a touch controller.

This may be used for output for raw and reference data. Values may range from
0 to 255.

**Byte Order.**
Each cell is one byte.



.. flat-table::
    :header-rows:  0
    :stub-columns: 0
    :widths:       2 1 1 1 1

    * - start + 0:
      - R'\ :sub:`00`
      - R'\ :sub:`01`
      - R'\ :sub:`02`
      - R'\ :sub:`03`
    * - start + 4:
      - R'\ :sub:`10`
      - R'\ :sub:`11`
      - R'\ :sub:`12`
      - R'\ :sub:`13`
    * - start + 8:
      - R'\ :sub:`20`
      - R'\ :sub:`21`
      - R'\ :sub:`22`
      - R'\ :sub:`23`
    * - start + 12:
      - R'\ :sub:`30`
      - R'\ :sub:`31`
      - R'\ :sub:`32`
      - R'\ :sub:`33`
