* Panasonic AMG88xx

The Panasonic family of AMG88xx Grid-Eye sensors allow recording
8x8 10Hz video which consists of thermal datapoints

Required Properties:
 - compatible : Must be "panasonic,amg88xx"
 - reg : i2c address of the device

Example:

	i2c0@1c22000 {
		...
		amg88xx@69 {
			compatible = "panasonic,amg88xx";
			reg = <0x69>;
		};
		...
	};
