Mediatek imgsys controller
============================

The Mediatek imgsys controller provides various clocks to the system.

Required Properties:

- compatible: Should be one of:
	- "mediatek,mt2701-imgsys", "syscon"
	- "mediatek,mt2712-imgsys", "syscon"
	- "mediatek,mt6765-imgsys", "syscon"
	- "mediatek,mt6779-imgsys", "syscon"
	- "mediatek,mt6797-imgsys", "syscon"
	- "mediatek,mt7623-imgsys", "mediatek,mt2701-imgsys", "syscon"
	- "mediatek,mt8167-imgsys", "syscon"
	- "mediatek,mt8173-imgsys", "syscon"
	- "mediatek,mt8183-imgsys", "syscon"
- #clock-cells: Must be 1

The imgsys controller uses the common clk binding from
Documentation/devicetree/bindings/clock/clock-bindings.txt
The available clocks are defined in dt-bindings/clock/mt*-clk.h.

Example:

imgsys: clock-controller@15000000 {
	compatible = "mediatek,mt8173-imgsys", "syscon";
	reg = <0 0x15000000 0 0x1000>;
	#clock-cells = <1>;
};
