Chinese translated version of Documentation/driver-api/io_ordering.rst

If you have any comment or update to the content, please contact the
original document maintainer directly.  However, if you have a problem
communicating in English you can also ask the Chinese maintainer for
help.  Contact the Chinese maintainer if this translation is outdated
or if there is a problem with the translation.

Traditional Chinese maintainer: Hu Haowen <2023002089@link.tyut.edu.cn>
---------------------------------------------------------------------
Documentation/driver-api/io_ordering.rst 的繁體中文翻譯

如果想評論或更新本文的內容，請直接聯繫原文檔的維護者。如果你使用英文
交流有困難的話，也可以向繁體中文版維護者求助。如果本翻譯更新不及時或
者翻譯存在問題，請聯繫繁體中文版維護者。

繁體中文版維護者： 胡皓文 Hu Haowen <2023002089@link.tyut.edu.cn>
繁體中文版翻譯者： 胡皓文 Hu Haowen <2023002089@link.tyut.edu.cn>
繁體中文版校譯者： 胡皓文 Hu Haowen <2023002089@link.tyut.edu.cn>


以下爲正文
---------------------------------------------------------------------

在某些平台上，所謂的內存映射I/O是弱順序。在這些平台上，驅動開發者有責任
保證I/O內存映射地址的寫操作按程序圖意的順序達到設備。通常讀取一個「安全」
設備寄存器或橋寄存器，觸發IO晶片清刷未處理的寫操作到達設備後才處理讀操作，
而達到保證目的。驅動程序通常在spinlock保護的臨界區退出之前使用這種技術。
這也可以保證後面的寫操作只在前面的寫操作之後到達設備（這非常類似於內存
屏障操作，mb()，不過僅適用於I/O）。

假設一個設備驅動程的具體例子：

        ...
CPU A:  spin_lock_irqsave(&dev_lock, flags)
CPU A:  val = readl(my_status);
CPU A:  ...
CPU A:  writel(newval, ring_ptr);
CPU A:  spin_unlock_irqrestore(&dev_lock, flags)
        ...
CPU B:  spin_lock_irqsave(&dev_lock, flags)
CPU B:  val = readl(my_status);
CPU B:  ...
CPU B:  writel(newval2, ring_ptr);
CPU B:  spin_unlock_irqrestore(&dev_lock, flags)
        ...

上述例子中，設備可能會先接收到newval2的值，然後接收到newval的值，問題就
發生了。不過很容易通過下面方法來修復：

        ...
CPU A:  spin_lock_irqsave(&dev_lock, flags)
CPU A:  val = readl(my_status);
CPU A:  ...
CPU A:  writel(newval, ring_ptr);
CPU A:  (void)readl(safe_register); /* 配置寄存器？*/
CPU A:  spin_unlock_irqrestore(&dev_lock, flags)
        ...
CPU B:  spin_lock_irqsave(&dev_lock, flags)
CPU B:  val = readl(my_status);
CPU B:  ...
CPU B:  writel(newval2, ring_ptr);
CPU B:  (void)readl(safe_register); /* 配置寄存器？*/
CPU B:  spin_unlock_irqrestore(&dev_lock, flags)

在解決方案中，讀取safe_register寄存器，觸發IO晶片清刷未處理的寫操作，
再處理後面的讀操作，防止引發數據不一致問題。

