# SPDX-License-Identifier: GPL-2.0

digraph board {
	rankdir=TB
	n00000001 [label="{{<port0> 0} | msm_csiphy0\n/dev/v4l-subdev0 | {<port1> 1}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000001:port1 -> n00000007:port0 [style=dashed]
	n00000001:port1 -> n0000000a:port0 [style=dashed]
	n00000004 [label="{{<port0> 0} | msm_csiphy1\n/dev/v4l-subdev1 | {<port1> 1}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000004:port1 -> n00000007:port0 [style=dashed]
	n00000004:port1 -> n0000000a:port0 [style=dashed]
	n00000007 [label="{{<port0> 0} | msm_csid0\n/dev/v4l-subdev2 | {<port1> 1}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000007:port1 -> n0000000d:port0 [style=dashed]
	n00000007:port1 -> n00000010:port0 [style=dashed]
	n0000000a [label="{{<port0> 0} | msm_csid1\n/dev/v4l-subdev3 | {<port1> 1}}", shape=Mrecord, style=filled, fillcolor=green]
	n0000000a:port1 -> n0000000d:port0 [style=dashed]
	n0000000a:port1 -> n00000010:port0 [style=dashed]
	n0000000d [label="{{<port0> 0} | msm_ispif0\n/dev/v4l-subdev4 | {<port1> 1}}", shape=Mrecord, style=filled, fillcolor=green]
	n0000000d:port1 -> n00000013:port0 [style=dashed]
	n0000000d:port1 -> n0000001c:port0 [style=dashed]
	n0000000d:port1 -> n00000025:port0 [style=dashed]
	n0000000d:port1 -> n0000002e:port0 [style=dashed]
	n00000010 [label="{{<port0> 0} | msm_ispif1\n/dev/v4l-subdev5 | {<port1> 1}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000010:port1 -> n00000013:port0 [style=dashed]
	n00000010:port1 -> n0000001c:port0 [style=dashed]
	n00000010:port1 -> n00000025:port0 [style=dashed]
	n00000010:port1 -> n0000002e:port0 [style=dashed]
	n00000013 [label="{{<port0> 0} | msm_vfe0_rdi0\n/dev/v4l-subdev6 | {<port1> 1}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000013:port1 -> n00000016 [style=bold]
	n00000016 [label="msm_vfe0_video0\n/dev/video0", shape=box, style=filled, fillcolor=yellow]
	n0000001c [label="{{<port0> 0} | msm_vfe0_rdi1\n/dev/v4l-subdev7 | {<port1> 1}}", shape=Mrecord, style=filled, fillcolor=green]
	n0000001c:port1 -> n0000001f [style=bold]
	n0000001f [label="msm_vfe0_video1\n/dev/video1", shape=box, style=filled, fillcolor=yellow]
	n00000025 [label="{{<port0> 0} | msm_vfe0_rdi2\n/dev/v4l-subdev8 | {<port1> 1}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000025:port1 -> n00000028 [style=bold]
	n00000028 [label="msm_vfe0_video2\n/dev/video2", shape=box, style=filled, fillcolor=yellow]
	n0000002e [label="{{<port0> 0} | msm_vfe0_pix\n/dev/v4l-subdev9 | {<port1> 1}}", shape=Mrecord, style=filled, fillcolor=green]
	n0000002e:port1 -> n00000031 [style=bold]
	n00000031 [label="msm_vfe0_video3\n/dev/video3", shape=box, style=filled, fillcolor=yellow]
	n00000057 [label="{{} | ov5645 1-0076\n/dev/v4l-subdev10 | {<port0> 0}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000057:port0 -> n00000001:port0 [style=bold]
	n00000059 [label="{{} | ov5645 1-0074\n/dev/v4l-subdev11 | {<port0> 0}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000059:port0 -> n00000004:port0 [style=bold]
}
