Maxim Integrated MAX3355 USB OTG chip
-------------------------------------

MAX3355 integrates a charge pump and comparators to enable a system with an
integrated USB OTG dual-role transceiver to function as a USB OTG dual-role
device.

Required properties:
- compatible: should be "maxim,max3355";
- maxim,shdn-gpios: should contain a phandle and GPIO specifier for the GPIO pin
		    connected to the MAX3355's SHDN# pin;
- id-gpios: should contain a phandle and GPIO specifier for the GPIO pin
	    connected to the MAX3355's ID_OUT pin.

Example:

	usb-otg {
		compatible = "maxim,max3355";
		maxim,shdn-gpios = <&gpio2 4 GPIO_ACTIVE_LOW>;
		id-gpios = <&gpio5 31 GPIO_ACTIVE_HIGH>;
	};
