What:		/sys/kernel/debug/moxtet/input
Date:		March 2019
KernelVersion:	5.3
Contact:	Marek Behún <kabel@kernel.org>
Description:	(Read) Read input from the shift registers, in hexadecimal.
		Returns N+1 bytes, where N is the number of Moxtet connected
		modules. The first byte is from the CPU board itself.

		Example::

			101214

		==  =======================================
		10  CPU board with SD card
		12  2 = PCIe module, 1 = IRQ not active
		14  4 = Peridot module, 1 = IRQ not active
		==  =======================================

What:		/sys/kernel/debug/moxtet/output
Date:		March 2019
KernelVersion:	5.3
Contact:	Marek Behún <kabel@kernel.org>
Description:	(RW) Read last written value to the shift registers, in
		hexadecimal, or write values to the shift registers, also
		in hexadecimal.

		Example::

		    0102

		==  ================================================
		01  01 was last written, or is to be written, to the
		    first module's shift register
		02  the same for second module
		==  ================================================
