* Kirkwood Thermal

This version is for Kirkwood 88F8262 & 88F6283 SoCs. Other kirkwoods
don't contain a thermal sensor.

Required properties:
- compatible : "marvell,kirkwood-thermal"
- reg : Address range of the thermal registers

Example:

	thermal@10078 {
		compatible = "marvell,kirkwood-thermal";
		reg = <0x10078 0x4>;
	};
