# SPDX-License-Identifier: GPL-2.0

digraph board {
	rankdir=TB
	n00000001 [label="{{} | Sensor A\n/dev/v4l-subdev0 | {<port0> 0}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000001:port0 -> n00000005:port0 [style=bold]
	n00000001:port0 -> n0000000b [style=bold]
	n00000001 -> n00000002
	n00000002 [label="{{} | Lens A\n/dev/v4l-subdev5 | {<port0>}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000003 [label="{{} | Sensor B\n/dev/v4l-subdev1 | {<port0> 0}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000003:port0 -> n00000008:port0 [style=bold]
	n00000003:port0 -> n0000000f [style=bold]
	n00000003 -> n00000004
	n00000004 [label="{{} | Lens B\n/dev/v4l-subdev6 | {<port0>}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000005 [label="{{<port0> 0} | Debayer A\n/dev/v4l-subdev2 | {<port1> 1}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000005:port1 -> n00000015:port0
	n00000008 [label="{{<port0> 0} | Debayer B\n/dev/v4l-subdev3 | {<port1> 1}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000008:port1 -> n00000015:port0 [style=dashed]
	n0000000b [label="Raw Capture 0\n/dev/video0", shape=box, style=filled, fillcolor=yellow]
	n0000000f [label="Raw Capture 1\n/dev/video1", shape=box, style=filled, fillcolor=yellow]
	n00000013 [label="{{} | RGB/YUV Input\n/dev/v4l-subdev4 | {<port0> 0}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000013:port0 -> n00000015:port0 [style=dashed]
	n00000015 [label="{{<port0> 0} | Scaler\n/dev/v4l-subdev5 | {<port1> 1}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000015:port1 -> n00000018 [style=bold]
	n00000018 [label="RGB/YUV Capture\n/dev/video2", shape=box, style=filled, fillcolor=yellow]
}
