* NVIDIA Tegra APB DMA controller

Required properties:
- compatible: Should be "nvidia,<chip>-apbdma"
- reg: Should contain DMA registers location and length. This should include
  all of the per-channel registers.
- interrupts: Should contain all of the per-channel DMA interrupts.
- clocks: Must contain one entry, for the module clock.
  See ../clocks/clock-bindings.txt for details.
- resets : Must contain an entry for each entry in reset-names.
  See ../reset/reset.txt for details.
- reset-names : Must include the following entries:
  - dma
- #dma-cells : Must be <1>. This dictates the length of DMA specifiers in
  client nodes' dmas properties. The specifier represents the DMA request
  select value for the peripheral. For more details, consult the Tegra TRM's
  documentation of the APB DMA channel control register REQ_SEL field.

Examples:

apbdma: dma@6000a000 {
	compatible = "nvidia,tegra20-apbdma";
	reg = <0x6000a000 0x1200>;
	interrupts = < 0 136 0x04
		       0 137 0x04
		       0 138 0x04
		       0 139 0x04
		       0 140 0x04
		       0 141 0x04
		       0 142 0x04
		       0 143 0x04
		       0 144 0x04
		       0 145 0x04
		       0 146 0x04
		       0 147 0x04
		       0 148 0x04
		       0 149 0x04
		       0 150 0x04
		       0 151 0x04 >;
	clocks = <&tegra_car 34>;
	resets = <&tegra_car 34>;
	reset-names = "dma";
	#dma-cells = <1>;
};
