What:		/sys/devices/platform/ts5500/adc
Date:		January 2013
KernelVersion:	3.7
Contact:	"Savoir-faire Linux Inc." <kernel@savoirfairelinux.com>
Description:
		Indicates the presence of an A/D Converter. If it is present,
		it will display "1", otherwise "0".

What:		/sys/devices/platform/ts5500/ereset
Date:		January 2013
KernelVersion:	3.7
Contact:	"Savoir-faire Linux Inc." <kernel@savoirfairelinux.com>
Description:
		Indicates the presence of an external reset. If it is present,
		it will display "1", otherwise "0".

What:		/sys/devices/platform/ts5500/id
Date:		January 2013
KernelVersion:	3.7
Contact:	"Savoir-faire Linux Inc." <kernel@savoirfairelinux.com>
Description:
		Product ID of the TS board. TS-5500 ID is 0x60.

What:		/sys/devices/platform/ts5500/jumpers
Date:		January 2013
KernelVersion:	3.7
Contact:	"Savoir-faire Linux Inc." <kernel@savoirfairelinux.com>
Description:
		Bitfield showing the jumpers' state. If a jumper is present,
		the corresponding bit is set. For instance, 0x0e means jumpers
		2, 3 and 4 are set.

What:		/sys/devices/platform/ts5500/name
Date:		July 2014
KernelVersion:	3.16
Contact:	"Savoir-faire Linux Inc." <kernel@savoirfairelinux.com>
Description:
		Model name of the TS board, e.g. "TS-5500".

What:		/sys/devices/platform/ts5500/rs485
Date:		January 2013
KernelVersion:	3.7
Contact:	"Savoir-faire Linux Inc." <kernel@savoirfairelinux.com>
Description:
		Indicates the presence of the RS485 option. If it is present,
		it will display "1", otherwise "0".

What:		/sys/devices/platform/ts5500/sram
Date:		January 2013
KernelVersion:	3.7
Contact:	"Savoir-faire Linux Inc." <kernel@savoirfairelinux.com>
Description:
		Indicates the presence of the SRAM option. If it is present,
		it will display "1", otherwise "0".
