Chinese translated version of Documentation/core-api/irq/index.rst

If you have any comment or update to the content, please contact the
original document maintainer directly.  However, if you have a problem
communicating in English you can also ask the Chinese maintainer for
help.  Contact the Chinese maintainer if this translation is outdated
or if there is a problem with the translation.

Maintainer: Eric W. Biederman <ebiederman@xmission.com>
Traditional Chinese maintainer: Hu Haowen <src.res.211@gmail.com>
---------------------------------------------------------------------
Documentation/core-api/irq/index.rst 的繁體中文翻譯

如果想評論或更新本文的內容，請直接聯繫原文檔的維護者。如果你使用英文
交流有困難的話，也可以向繁體中文版維護者求助。如果本翻譯更新不及時或
者翻譯存在問題，請聯繫繁體中文版維護者。

英文版維護者： Eric W. Biederman <ebiederman@xmission.com>
繁體中文版維護者： 胡皓文 Hu Haowen <src.res.211@gmail.com>
繁體中文版翻譯者： 胡皓文 Hu Haowen <src.res.211@gmail.com>
繁體中文版校譯者： 胡皓文 Hu Haowen <src.res.211@gmail.com>


以下爲正文
---------------------------------------------------------------------
何爲 IRQ?

一個 IRQ 是來自某個設備的一個中斷請求。目前，它們可以來自一個硬體引腳，
或來自一個數據包。多個設備可能連接到同個硬體引腳，從而共享一個 IRQ。

一個 IRQ 編號是用於告知硬體中斷源的內核標識。通常情況下，這是一個
全局 irq_desc 數組的索引，但是除了在 linux/interrupt.h 中的實現，
具體的細節是體系結構特定的。

一個 IRQ 編號是設備上某個可能的中斷源的枚舉。通常情況下，枚舉的編號是
該引腳在系統內中斷控制器的所有輸入引腳中的編號。對於 ISA 總線中的情況，
枚舉的是在兩個 i8259 中斷控制器中 16 個輸入引腳。

架構可以對 IRQ 編號指定額外的含義，在硬體涉及任何手工配置的情況下，
是被提倡的。ISA 的 IRQ 是一個分配這類額外含義的典型例子。

