max8925-battery bindings
~~~~~~~~~~~~~~~~

Optional properties :
 - batt-detect: whether support battery detect
 - topoff-threshold: set charging current in topoff mode
 - fast-charge: set charging current in fast mode
 - no-temp-support: whether support temperature protection detect
 - no-insert-detect: whether support insert detect

Example:
	charger {
		batt-detect = <0>;
		topoff-threshold = <1>;
		fast-charge = <7>;
		no-temp-support = <0>;
		no-insert-detect = <0>;
	};
