Realtek RTD1295 Watchdog
========================

Required properties:

- compatible :  Should be "realtek,rtd1295-watchdog"
- reg        :  Specifies the physical base address and size of registers
- clocks     :  Specifies one clock input


Example:

	watchdog@98007680 {
		compatible = "realtek,rtd1295-watchdog";
		reg = <0x98007680 0x100>;
		clocks = <&osc27M>;
	};
