Marvell Armada 38x Platforms Device Tree Bindings
-------------------------------------------------

Boards with a SoC of the Marvell Armada 38x family shall have the
following property:

Required root node property:

 - compatible: must contain "marvell,armada380"

In addition, boards using the Marvell Armada 385 SoC shall have the
following property before the previous one:

Required root node property:

compatible: must contain "marvell,armada385"

In addition, boards using the Marvell Armada 388 SoC shall have the
following property before the previous one:

Required root node property:

compatible: must contain "marvell,armada388"

Example:

compatible = "marvell,a385-rd", "marvell,armada385", "marvell,armada380";
