Amlogic Meson6/Meson8/Meson8b assist registers:
-----------------------------------------------

The assist registers contain basic information about the SoC,
for example the encoded SoC part number.

Required properties:
- reg: the register range of the assist registers
- compatible: should be "amlogic,meson-mx-assist" along with "syscon"


Example:

	assist: assist@7c00 {
		compatible = "amlogic,meson-mx-assist", "syscon";
		reg = <0x7c00 0x200>;
	};
