What:		/sys/class/misc/drivers/dw-xdata-pcie.<device>/write
Date:		April 2021
KernelVersion:	5.13
Contact:	Gustavo Pimentel <gustavo.pimentel@synopsys.com>
Description:	Allows the user to enable the PCIe traffic generator which
		will create write TLPs frames - from the Root Complex to the
		Endpoint direction or to disable the PCIe traffic generator
		in all directions.

		Write y/1/on to enable, n/0/off to disable

		Usage e.g.
		 echo 1 > /sys/class/misc/dw-xdata-pcie.<device>/write
		or
		 echo 0 > /sys/class/misc/dw-xdata-pcie.<device>/write

		The user can read the current PCIe link throughput generated
		through this generator in MB/s.

		Usage e.g.
		 cat /sys/class/misc/dw-xdata-pcie.<device>/write
		 204

		The file is read and write.

What:		/sys/class/misc/dw-xdata-pcie.<device>/read
Date:		April 2021
KernelVersion:	5.13
Contact:	Gustavo Pimentel <gustavo.pimentel@synopsys.com>
Description:	Allows the user to enable the PCIe traffic generator which
		will create read TLPs frames - from the Endpoint to the Root
		Complex direction or to disable the PCIe traffic generator
                in all directions.

		Write y/1/on to enable, n/0/off to disable

		Usage e.g.
		 echo 1 > /sys/class/misc/dw-xdata-pcie.<device>/read
		or
		 echo 0 > /sys/class/misc/dw-xdata-pcie.<device>/read

		The user can read the current PCIe link throughput generated
		through this generator in MB/s.

		Usage e.g.
		 cat /sys/class/misc/dw-xdata-pcie.<device>/read
		 199

		The file is read and write.
