# SPDX-License-Identifier: GPL-2.0

digraph board {
	rankdir=TB
	colorscheme=x11
	scaler [label="{<scaler_0> 0} | Host\nScaler | {<scaler_1> 1} ", shape=Mrecord, style=filled, fillcolor=lightblue]
	frontend [label="{<frontend_0> 0} | Host\nFrontend | {<frontend_1> 1}", shape=Mrecord, style=filled, fillcolor=lightblue]
	sensor [label="Sensor | {<sensor_0> 0}", shape=Mrecord, style=filled, fillcolor=aquamarine]
	io [label="{<io_0> 0} | V4L I/O", shape=Mrecord, style=filled, fillcolor=aquamarine]

	sensor:sensor_0 -> frontend:frontend_0 [color=blue, label="HQ: 2592x1968\nHS: 1296x984"]
	frontend:frontend_1 -> scaler:scaler_0 [color=blue, label="HQ: 2592x1968\nHS: 1296x984"]
	scaler:scaler_1 -> io:io_0 [color=blue, label="HQ: 1280x720\nHS: 1280x720"]
}
