.. SPDX-License-Identifier: GFDL-1.1-no-invariants-or-later

.. _V4L2-PIX-FMT-SRGGB14P:
.. _v4l2-pix-fmt-sbggr14p:
.. _v4l2-pix-fmt-sgbrg14p:
.. _v4l2-pix-fmt-sgrbg14p:

*******************************************************************************************************************************
V4L2_PIX_FMT_SRGGB14P ('pREE'), V4L2_PIX_FMT_SGRBG14P ('pgEE'), V4L2_PIX_FMT_SGBRG14P ('pGEE'), V4L2_PIX_FMT_SBGGR14P ('pBEE'),
*******************************************************************************************************************************

*man V4L2_PIX_FMT_SRGGB14P(2)*

V4L2_PIX_FMT_SGRBG14P
V4L2_PIX_FMT_SGBRG14P
V4L2_PIX_FMT_SBGGR14P
14-bit packed Bayer formats


Description
===========

These four pixel formats are packed raw sRGB / Bayer formats with 14
bits per colour. Every four consecutive samples are packed into seven
bytes. Each of the first four bytes contain the eight high order bits
of the pixels, and the three following bytes contains the six least
significants bits of each pixel, in the same order.

Each n-pixel row contains n/2 green samples and n/2 blue or red samples,
with alternating green-red and green-blue rows. They are conventionally
described as GRGR... BGBG..., RGRG... GBGB..., etc. Below is an example
of one of these formats:

**Byte Order.**
Each cell is one byte.

.. raw:: latex

    \begingroup
    \footnotesize
    \setlength{\tabcolsep}{2pt}

.. tabularcolumns:: |p{1.6cm}|p{1.0cm}|p{1.0cm}|p{1.0cm}|p{1.0cm}|p{3.5cm}|p{3.5cm}|p{3.5cm}|

.. flat-table::
    :header-rows:  0
    :stub-columns: 0
    :widths:       2 1 1 1 1 3 3 3


    -  .. row 1

       -  start + 0

       -  B\ :sub:`00high`

       -  G\ :sub:`01high`

       -  B\ :sub:`02high`

       -  G\ :sub:`03high`

       -  G\ :sub:`01low bits 1--0`\ (bits 7--6)

	  B\ :sub:`00low bits 5--0`\ (bits 5--0)

       -  B\ :sub:`02low bits 3--0`\ (bits 7--4)

	  G\ :sub:`01low bits 5--2`\ (bits 3--0)

       -  G\ :sub:`03low bits 5--0`\ (bits 7--2)

	  B\ :sub:`02low bits 5--4`\ (bits 1--0)

    -  .. row 2

       -  start + 7

       -  G\ :sub:`10high`

       -  R\ :sub:`11high`

       -  G\ :sub:`12high`

       -  R\ :sub:`13high`

       -  R\ :sub:`11low bits 1--0`\ (bits 7--6)

	  G\ :sub:`10low bits 5--0`\ (bits 5--0)

       -  G\ :sub:`12low bits 3--0`\ (bits 7--4)

	  R\ :sub:`11low bits 5--2`\ (bits 3--0)

       -  R\ :sub:`13low bits 5--0`\ (bits 7--2)

	  G\ :sub:`12low bits 5--4`\ (bits 1--0)

    -  .. row 3

       -  start + 14

       -  B\ :sub:`20high`

       -  G\ :sub:`21high`

       -  B\ :sub:`22high`

       -  G\ :sub:`23high`

       -  G\ :sub:`21low bits 1--0`\ (bits 7--6)

	  B\ :sub:`20low bits 5--0`\ (bits 5--0)

       -  B\ :sub:`22low bits 3--0`\ (bits 7--4)

	  G\ :sub:`21low bits 5--2`\ (bits 3--0)

       -  G\ :sub:`23low bits 5--0`\ (bits 7--2)

	  B\ :sub:`22low bits 5--4`\ (bits 1--0)

    -  .. row 4

       -  start + 21

       -  G\ :sub:`30high`

       -  R\ :sub:`31high`

       -  G\ :sub:`32high`

       -  R\ :sub:`33high`

       -  R\ :sub:`31low bits 1--0`\ (bits 7--6)
	  G\ :sub:`30low bits 5--0`\ (bits 5--0)

       -  G\ :sub:`32low bits 3--0`\ (bits 7--4)
	  R\ :sub:`31low bits 5--2`\ (bits 3--0)

       -  R\ :sub:`33low bits 5--0`\ (bits 7--2)
	  G\ :sub:`32low bits 5--4`\ (bits 1--0)

.. raw:: latex

    \endgroup

